;; GCC machine description for Hitachi H8/300
;; Copyright (C) 1992, 1993, 1994, 1995, 1996, 1997, 1998, 1999, 2000,
;; 2001, 2002, 2003 Free Software Foundation, Inc.

;;   Contributed by Steve Chamberlain (sac@cygnus.com),
;;   Jim Wilson (wilson@cygnus.com), and Doug Evans (dje@cygnus.com).

;; This file is part of GNU CC.

;; GNU CC is free software; you can redistribute it and/or modify
;; it under the terms of the GNU General Public License as published by
;; the Free Software Foundation; either version 2, or (at your option)
;; any later version.

;; GNU CC is distributed in the hope that it will be useful,
;; but WITHOUT ANY WARRANTY; without even the implied warranty of
;; MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
;; GNU General Public License for more details.

;; You should have received a copy of the GNU General Public License
;; along with GNU CC; see the file COPYING.  If not, write to
;; the Free Software Foundation, 59 Temple Place - Suite 330,
;; Boston, MA 02111-1307, USA.

;; Some of the extend instructions accept a general_operand_src, which
;; allows all the normal memory addressing modes.  The length computations
;; don't take this into account.  The lengths in the MD file should be
;; "worst case" and then be adjusted to their correct values by
;; h8300_adjust_insn_length.

;; On the H8/300H and H8S, adds/subs operate on the 32bit "er"
;; registers.  Right now GCC doesn't expose the "e" half to the
;; compiler, so using add/subs for addhi and subhi is safe.  Long
;; term, we want to expose the "e" half to the compiler (gives us 8
;; more 16bit registers).  At that point addhi and subhi can't use
;; adds/subs.

;; There's currently no way to have an insv/extzv expander for the H8/300H
;; because word_mode is different for the H8/300 and H8/300H.

;; Shifts/rotates by small constants should be handled by special
;; patterns so we get the length and cc status correct.

;; Bitfield operations no longer accept memory operands.  We need
;; to add variants which operate on memory back to the MD.

;; ??? Implement remaining bit ops available on the h8300

;; ----------------------------------------------------------------------
;; CONSTANTS
;; ----------------------------------------------------------------------

(define_constants
  [(SC_REG	 3)
   (FP_REG	 6)
   (SP_REG	 7)
   (MAC_REG	 8)
   (AP_REG	 9)
   (RAP_REG	10)])

;; ----------------------------------------------------------------------
;; ATTRIBUTES
;; ----------------------------------------------------------------------

(define_attr "cpu" "h8300,h8300h"
  (const (symbol_ref "cpu_type")))

(define_attr "type" "branch,arith"
  (const_string "arith"))

;; The size of instructions in bytes.

(define_attr "length" ""
  (cond [(eq_attr "type" "branch")
	 (if_then_else (and (ge (minus (match_dup 0) (pc))
				(const_int -126))
			    (le (minus (match_dup 0) (pc))
				(const_int 126)))
		       (const_int 2)
		       (if_then_else (and (eq_attr "cpu" "h8300h")
					  (and (ge (minus (pc) (match_dup 0))
						   (const_int -32000))
					       (le (minus (pc) (match_dup 0))
						   (const_int 32000))))
				     (const_int 4)
				     (const_int 6)))]
	(const_int 200)))

;; The necessity of instruction length adjustment.

(define_attr "adjust_length" "yes,no"
  (cond [(eq_attr "type" "branch") (const_string "no")]
	(const_string "yes")))

;; Condition code settings.
;;
;; none - insn does not affect cc
;; none_0hit - insn does not affect cc but it does modify operand 0
;;	This attribute is used to keep track of when operand 0 changes.
;;	See the description of NOTICE_UPDATE_CC for more info.
;; set_znv - insn sets z,n,v to usable values (like a tst insn); c is unknown.
;; set_zn  - insn sets z,n to usable values; v,c are unknown.
;; compare - compare instruction
;; clobber - value of cc is unknown

(define_attr "cc" "none,none_0hit,set_znv,set_zn,compare,clobber"
  (const_string "clobber"))

;; ----------------------------------------------------------------------
;; MOVE INSTRUCTIONS
;; ----------------------------------------------------------------------

;; movqi

(define_insn "pushqi1_h8300"
  [(parallel [(set (reg:HI SP_REG)
		   (plus:HI (reg:HI SP_REG) (const_int -2)))
	      (set (mem:QI (plus:HI (reg:HI SP_REG) (const_int -1)))
		   (match_operand:QI 0 "register_operand" "r"))])]
  "TARGET_H8300
   && REGNO (operands[0]) != SP_REG"
  "mov.w\\t%T0,@-r7"
  [(set_attr "length" "2")
   (set_attr "cc" "clobber")])

(define_insn "pushqi1_h8300hs"
  [(parallel [(set (reg:SI SP_REG)
		   (plus:SI (reg:SI SP_REG) (const_int -4)))
	      (set (mem:QI (plus:SI (reg:SI SP_REG) (const_int -3)))
		   (match_operand:QI 0 "register_operand" "r"))])]
  "(TARGET_H8300H || TARGET_H8300S)
   && REGNO (operands[0]) != SP_REG"
  "mov.l\\t%S0,@-er7"
  [(set_attr "length" "4")
   (set_attr "cc" "clobber")])

(define_expand "pushqi1"
  [(use (match_operand:QI 0 "register_operand" ""))]
  ""
  "
{
  if (TARGET_H8300)
    emit_insn (gen_pushqi1_h8300 (operands[0]));
  else
    emit_insn (gen_pushqi1_h8300hs (operands[0]));
  DONE;
}")

(define_insn ""
  [(set (match_operand:QI 0 "general_operand_dst" "=r,r ,<,r,r,m")
	(match_operand:QI 1 "general_operand_src" " I,r>,r,n,m,r"))]
  "TARGET_H8300
   && (register_operand (operands[0], QImode)
       || register_operand (operands[1], QImode))"
  "@
   sub.b	%X0,%X0
   mov.b	%R1,%X0
   mov.b	%X1,%R0
   mov.b	%R1,%X0
   mov.b	%R1,%X0
   mov.b	%X1,%R0"
  [(set_attr "length" "2,2,2,2,4,4")
   (set_attr "cc" "set_zn,set_znv,set_znv,set_znv,set_znv,set_znv")])

(define_insn ""
  [(set (match_operand:QI 0 "general_operand_dst" "=r,r ,<,r,r,m")
	(match_operand:QI 1 "general_operand_src" " I,r>,r,n,m,r"))]
  "(TARGET_H8300H || TARGET_H8300S)
   && (register_operand (operands[0], QImode)
       || register_operand (operands[1], QImode))"
  "@
   sub.b	%X0,%X0
   mov.b	%R1,%X0
   mov.b	%X1,%R0
   mov.b	%R1,%X0
   mov.b	%R1,%X0
   mov.b	%X1,%R0"
  [(set_attr "length" "2,2,2,2,8,8")
   (set_attr "cc" "set_zn,set_znv,set_znv,clobber,set_znv,set_znv")])

(define_expand "movqi"
  [(set (match_operand:QI 0 "general_operand_dst" "")
	(match_operand:QI 1 "general_operand_src" ""))]
  ""
  "
{
  /* One of the ops has to be in a register.  */
  if (!register_operand (operand0, QImode)
      && !register_operand (operand1, QImode))
    {
      operands[1] = copy_to_mode_reg (QImode, operand1);
    }
}")

(define_insn "movstrictqi"
  [(set (strict_low_part (match_operand:QI 0 "general_operand_dst" "+r,r,r,r"))
			 (match_operand:QI 1 "general_operand_src" "I,r,n,m"))]
  ""
  "@
   sub.b	%X0,%X0
   mov.b	%X1,%X0
   mov.b	%R1,%X0
   mov.b	%R1,%X0"
  [(set_attr_alternative "length"
     [(const_int 2) (const_int 2) (const_int 2)
      (if_then_else (eq_attr "cpu" "h8300") (const_int 4) (const_int 8))])
   (set_attr "cc" "set_zn,set_znv,set_znv,set_znv")])

;; movhi

(define_expand "pushhi1_h8300"
  [(set (mem:HI (pre_dec:HI (reg:HI SP_REG)))
	(match_operand:HI 0 "register_operand" ""))]
  "TARGET_H8300
   && REGNO (operands[0]) != SP_REG"
  "")

(define_insn "pushhi1_h8300hs"
  [(parallel [(set (reg:SI SP_REG)
		   (plus:SI (reg:SI SP_REG) (const_int -4)))
	      (set (mem:HI (plus:SI (reg:SI SP_REG) (const_int -2)))
		   (match_operand:HI 0 "register_operand" "r"))])]
  "(TARGET_H8300H || TARGET_H8300S)
   && REGNO (operands[0]) != SP_REG"
  "mov.l\\t%S0,@-er7"
  [(set_attr "length" "4")
   (set_attr "cc" "clobber")])

(define_expand "pushhi1"
  [(use (match_operand:HI 0 "register_operand" ""))]
  ""
  "
{
  if (TARGET_H8300)
    emit_insn (gen_pushhi1_h8300 (operands[0]));
  else
    emit_insn (gen_pushhi1_h8300hs (operands[0]));
  DONE;
}")

(define_insn ""
  [(set (match_operand:HI 0 "general_operand_dst" "=r,r,<,r,r,m")
	(match_operand:HI 1 "general_operand_src" "I,r>,r,i,m,r"))]
  "TARGET_H8300
   && (register_operand (operands[0], HImode)
       || register_operand (operands[1], HImode))
   && !(GET_CODE (operands[0]) == MEM
	&& GET_CODE (XEXP (operands[0], 0)) == PRE_DEC
	&& GET_CODE (XEXP (XEXP (operands[0], 0), 0)) == REG
	&& GET_CODE (operands[1]) == REG
	&& REGNO (XEXP (XEXP (operands[0], 0), 0)) == REGNO (operands[1]))"
  "@
   sub.w	%T0,%T0
   mov.w	%T1,%T0
   mov.w	%T1,%T0
   mov.w	%T1,%T0
   mov.w	%T1,%T0
   mov.w	%T1,%T0"
  [(set_attr "length" "2,2,2,4,4,4")
   (set_attr "cc" "set_zn,set_znv,set_znv,set_znv,set_znv,set_znv")])

(define_insn ""
  [(set (match_operand:HI 0 "general_operand_dst" "=r,r,<,r,r,m")
	(match_operand:HI 1 "general_operand_src" "I,r>,r,i,m,r"))]
  "(TARGET_H8300H || TARGET_H8300S)
   && (register_operand (operands[0], HImode)
       || register_operand (operands[1], HImode))"
  "@
   sub.w	%T0,%T0
   mov.w	%T1,%T0
   mov.w	%T1,%T0
   mov.w	%T1,%T0
   mov.w	%T1,%T0
   mov.w	%T1,%T0"
  [(set_attr "length" "2,2,2,4,8,8")
   (set_attr "cc" "set_zn,set_znv,set_znv,set_znv,set_znv,set_znv")])

(define_expand "movhi"
  [(set (match_operand:HI 0 "general_operand_dst" "")
	(match_operand:HI 1 "general_operand_src" ""))]
  ""
  "
{
  /* One of the ops has to be in a register.  */
  if (!register_operand (operand1, HImode)
      && !register_operand (operand0, HImode))
    {
      operands[1] = copy_to_mode_reg (HImode, operand1);
    }
}")

(define_insn "movstricthi"
  [(set (strict_low_part (match_operand:HI 0 "general_operand_dst" "+r,r,r,r"))
			 (match_operand:HI 1 "general_operand_src" "I,r,i,m"))]
  ""
  "@
   sub.w	%T0,%T0
   mov.w	%T1,%T0
   mov.w	%T1,%T0
   mov.w	%T1,%T0"
  [(set_attr_alternative "length"
     [(const_int 2) (const_int 2) (const_int 4)
      (if_then_else (eq_attr "cpu" "h8300") (const_int 4) (const_int 8))])
   (set_attr "cc" "set_zn,set_znv,set_znv,set_znv")])

;; movsi

(define_expand "movsi"
  [(set (match_operand:SI 0 "general_operand_dst" "")
	(match_operand:SI 1 "general_operand_src" ""))]
  ""
  "
{
  if (TARGET_H8300)
    {
      if (do_movsi (operands))
	DONE;
    }
  else
    {
      /* One of the ops has to be in a register.  */
      if (!register_operand (operand1, SImode)
	  && !register_operand (operand0, SImode))
	{
	  operands[1] = copy_to_mode_reg (SImode, operand1);
	}
    }
}")

(define_expand "movsf"
  [(set (match_operand:SF 0 "general_operand_dst" "")
	(match_operand:SF 1 "general_operand_src" ""))]
  ""
  "
{
  if (TARGET_H8300)
    {
      if (do_movsi (operands))
	DONE;
    }
  else
    {
      /* One of the ops has to be in a register.  */
      if (!register_operand (operand1, SFmode)
	  && !register_operand (operand0, SFmode))
	{
	  operands[1] = copy_to_mode_reg (SFmode, operand1);
	}
    }
}")

(define_insn "movsi_h8300"
  [(set (match_operand:SI 0 "general_operand_dst" "=r,r,r,o,<,r")
	(match_operand:SI 1 "general_operand_src" "I,r,io,r,r,>"))]
  "TARGET_H8300
   && (register_operand (operands[0], SImode)
       || register_operand (operands[1], SImode))"
  "*
{
  int rn = -1;
  switch (which_alternative)
    {
    case 0:
      return \"sub.w	%e0,%e0\;sub.w	%f0,%f0\";
    case 1:
      if (REGNO (operands[0]) < REGNO (operands[1]))
	return \"mov.w	%e1,%e0\;mov.w	%f1,%f0\";
      else
	return \"mov.w	%f1,%f0\;mov.w	%e1,%e0\";
    case 2:
      /* Make sure we don't trample the register we index with.  */
      if (GET_CODE (operands[1]) == MEM)
	{
	  rtx inside = XEXP (operands[1], 0);
	  if (REG_P (inside))
	    {
	      rn = REGNO (inside);
	    }
	  else if (GET_CODE (inside) == PLUS)
	    {
	      rtx lhs = XEXP (inside, 0);
	      rtx rhs = XEXP (inside, 1);
	      if (REG_P (lhs)) rn = REGNO (lhs);
	      if (REG_P (rhs)) rn = REGNO (rhs);
	    }
	}
      if (rn == REGNO (operands[0]))
	{
	  /* Move the second word first.  */
	  return \"mov.w	%f1,%f0\;mov.w	%e1,%e0\";
	}
      else
	{
	  /* See if either half is zero.  If so, use sub.w to clear
	     that half.  */
	  if (GET_CODE (operands[1]) == CONST_INT)
	    {
	      if ((INTVAL (operands[1]) & 0xffff) == 0)
		return \"mov.w	%e1,%e0\;sub.w	%f0,%f0\";
	      if (((INTVAL (operands[1]) >> 16) & 0xffff) == 0)
		return \"sub.w	%e0,%e0\;mov.w	%f1,%f0\";
	    }
	  return \"mov.w	%e1,%e0\;mov.w	%f1,%f0\";
	}
    case 3:
      return \"mov.w	%e1,%e0\;mov.w	%f1,%f0\";
    case 4:
      return \"mov.w	%f1,%T0\;mov.w	%e1,%T0\";
    case 5:
      return \"mov.w	%T1,%e0\;mov.w	%T1,%f0\";
    default:
      abort ();
    }
}"
  [(set_attr "length" "4,4,8,8,4,4")
   (set_attr "cc" "clobber")])

(define_insn "movsf_h8300"
  [(set (match_operand:SF 0 "general_operand_dst" "=r,r,r,o,<,r")
	(match_operand:SF 1 "general_operand_src" "I,r,io,r,r,>"))]
  "TARGET_H8300
   && (register_operand (operands[0], SFmode)
       || register_operand (operands[1], SFmode))"
  "*
{
  /* Copy of the movsi stuff.  */
  int rn = -1;
  switch (which_alternative)
    {
    case 0:
      return \"sub.w	%e0,%e0\;sub.w	%f0,%f0\";
    case 1:
      if (REGNO (operands[0]) < REGNO (operands[1]))
	return \"mov.w	%e1,%e0\;mov.w	%f1,%f0\";
      else
	return \"mov.w	%f1,%f0\;mov.w	%e1,%e0\";
    case 2:
      /* Make sure we don't trample the register we index with.  */
      if (GET_CODE (operands[1]) == MEM)
	{
	  rtx inside = XEXP (operands[1], 0);
	  if (REG_P (inside))
	    {
	      rn = REGNO (inside);
	    }
	  else if (GET_CODE (inside) == PLUS)
	    {
	      rtx lhs = XEXP (inside, 0);
	      rtx rhs = XEXP (inside, 1);
	      if (REG_P (lhs)) rn = REGNO (lhs);
	      if (REG_P (rhs)) rn = REGNO (rhs);
	    }
	}
      if (rn == REGNO (operands[0]))
	/* Move the second word first.  */
	return \"mov.w	%f1,%f0\;mov.w	%e1,%e0\";
      else
	/* Move the first word first.  */
	return \"mov.w	%e1,%e0\;mov.w	%f1,%f0\";

    case 3:
      return \"mov.w	%e1,%e0\;mov.w	%f1,%f0\";
    case 4:
      return \"mov.w	%f1,%T0\;mov.w	%e1,%T0\";
    case 5:
      return \"mov.w	%T1,%e0\;mov.w	%T1,%f0\";
    default:
      abort ();
    }
}"
  [(set_attr "length" "4,4,8,8,4,4")
   (set_attr "cc" "clobber")])

(define_insn "movsi_h8300hs"
  [(set (match_operand:SI 0 "general_operand_dst" "=r,r,r,<,r,r,m,*a,*a,r")
	(match_operand:SI 1 "general_operand_src" "I,r,i,r,>,m,r,I,r,*a"))]
  "(TARGET_H8300S || TARGET_H8300H)
   && (register_operand (operands[0], SImode)
       || register_operand (operands[1], SImode))
   && !(GET_CODE (operands[0]) == MEM
	&& GET_CODE (XEXP (operands[0], 0)) == PRE_DEC
	&& GET_CODE (XEXP (XEXP (operands[0], 0), 0)) == REG
	&& GET_CODE (operands[1]) == REG
	&& REGNO (XEXP (XEXP (operands[0], 0), 0)) == REGNO (operands[1]))"
  "*
{
  switch (which_alternative)
    {
    case 0:
      return \"sub.l	%S0,%S0\";
    case 7:
      return \"clrmac\";
    case 8:
      return \"clrmac\;ldmac %1,macl\";
    case 9:
      return \"stmac	macl,%0\";
    default:
      if (GET_CODE (operands[1]) == CONST_INT)
	{
	  int val = INTVAL (operands[1]);

	  /* Look for constants which can be made by adding an 8-bit
	     number to zero in one of the two low bytes.  */
	  if (val == (val & 0xff))
	    {
	      operands[1] = GEN_INT ((char) val & 0xff);
	      return \"sub.l\\t%S0,%S0\;add.b\\t%1,%w0\";
	    }

	  if (val == (val & 0xff00))
	    {
	      operands[1] = GEN_INT ((char) (val >> 8) & 0xff);
	      return \"sub.l\\t%S0,%S0\;add.b\\t%1,%x0\";
	    }

	  /* Look for constants that can be obtained by subs, inc, and
	     dec to 0.  */
	  switch (val & 0xffffffff)
	    {
	    case 0xffffffff:
	      return \"sub.l\\t%S0,%S0\;subs\\t#1,%S0\";
	    case 0xfffffffe:
	      return \"sub.l\\t%S0,%S0\;subs\\t#2,%S0\";
	    case 0xfffffffc:
	      return \"sub.l\\t%S0,%S0\;subs\\t#4,%S0\";

	    case 0x0000ffff:
	      return \"sub.l\\t%S0,%S0\;dec.w\\t#1,%f0\";
	    case 0x0000fffe:
	      return \"sub.l\\t%S0,%S0\;dec.w\\t#2,%f0\";

	    case 0xffff0000:
	      return \"sub.l\\t%S0,%S0\;dec.w\\t#1,%e0\";
	    case 0xfffe0000:
	      return \"sub.l\\t%S0,%S0\;dec.w\\t#2,%e0\";

	    case 0x00010000:
	      return \"sub.l\\t%S0,%S0\;inc.w\\t#1,%e0\";
	    case 0x00020000:
	      return \"sub.l\\t%S0,%S0\;inc.w\\t#2,%e0\";
	    }
	}
    }
   return \"mov.l	%S1,%S0\";
}"
  [(set_attr "length" "2,2,6,4,4,10,10,2,6,4")
   (set_attr "cc" "set_zn,set_znv,clobber,set_znv,set_znv,set_znv,set_znv,none_0hit,none_0hit,set_znv")])

(define_insn "movsf_h8300h"
  [(set (match_operand:SF 0 "general_operand_dst" "=r,r,r,m,<,r")
	(match_operand:SF 1 "general_operand_src" "I,r,im,r,r,>"))]
  "(TARGET_H8300H || TARGET_H8300S)
   && (register_operand (operands[0], SFmode)
       || register_operand (operands[1], SFmode))"
  "@
   sub.l	%S0,%S0
   mov.l	%S1,%S0
   mov.l	%S1,%S0
   mov.l	%S1,%S0
   mov.l	%S1,%S0
   mov.l	%S1,%S0"
  [(set_attr "length" "2,2,10,10,4,4")
   (set_attr "cc" "set_zn,set_znv,set_znv,set_znv,set_znv,set_znv")])

;; ----------------------------------------------------------------------
;; TEST INSTRUCTIONS
;; ----------------------------------------------------------------------

(define_insn ""
  [(set (cc0) (zero_extract:HI (match_operand:QI 0 "bit_memory_operand" "r,U")
			       (const_int 1)
			       (match_operand 1 "const_int_operand" "n,n")))]
  "TARGET_H8300"
  "btst	%Z1,%Y0"
  [(set_attr "length" "2,4")
   (set_attr "cc" "set_zn,set_zn")])

(define_insn ""
  [(set (cc0) (zero_extract:HI (match_operand:HI 0 "register_operand" "r")
			       (const_int 1)
			       (match_operand 1 "const_int_operand" "n")))]
  "TARGET_H8300"
  "btst	%Z1,%Y0"
  [(set_attr "length" "2")
   (set_attr "cc" "set_zn")])

(define_insn "*tst_extzv_bitqi_1_n"
  [(set (cc0) (zero_extract:SI (match_operand:QI 0 "bit_operand" "r,U")
			       (const_int 1)
			       (match_operand 1 "const_int_operand" "n,n")))]
  "(TARGET_H8300H || TARGET_H8300S)
   && INTVAL (operands[1]) != 7"
  "btst	%Z1,%Y0"
  [(set_attr "length" "2,8")
   (set_attr "cc" "set_zn,set_zn")])

(define_insn_and_split "*tst_extzv_memqi_1_n"
  [(set (cc0) (zero_extract:SI (match_operand:QI 0 "memory_operand" "m")
			       (const_int 1)
			       (match_operand 1 "const_int_operand" "n")))
   (clobber (match_scratch:QI 2 "=&r"))]
  "(TARGET_H8300H || TARGET_H8300S)
   && !EXTRA_CONSTRAINT (operands[0], 'U')
   && INTVAL (operands[1]) != 7"
  "#"
  "&& reload_completed"
  [(set (match_dup 2)
	(match_dup 0))
   (set (cc0) (zero_extract:SI (match_dup 2)
			       (const_int 1)
			       (match_dup 1)))]
  "")

(define_insn ""
  [(set (cc0) (zero_extract:SI (match_operand:SI 0 "register_operand" "r")
			       (const_int 1)
			       (match_operand 1 "const_int_operand" "n")))]
  "(TARGET_H8300H || TARGET_H8300S)
   && INTVAL (operands[1]) <= 15"
  "btst	%Z1,%Y0"
  [(set_attr "length" "2")
   (set_attr "cc" "set_zn")])

(define_insn "tstqi"
  [(set (cc0) (match_operand:QI 0 "register_operand" "r"))]
  ""
  "mov.b	%X0,%X0"
  [(set_attr "length" "2")
   (set_attr "cc" "set_znv")])

(define_insn "tsthi"
  [(set (cc0) (match_operand:HI 0 "register_operand" "r"))]
  ""
  "mov.w	%T0,%T0"
  [(set_attr "length" "2")
   (set_attr "cc" "set_znv")])

(define_insn ""
  [(set (cc0)
	(and:HI (match_operand:HI 0 "register_operand" "r")
		(const_int -256)))]
  ""
  "mov.b	%t0,%t0"
  [(set_attr "length" "2")
   (set_attr "cc" "set_znv")])

(define_insn "tstsi"
  [(set (cc0) (match_operand:SI 0 "register_operand" "r"))]
  "TARGET_H8300H || TARGET_H8300S"
  "mov.l	%S0,%S0"
  [(set_attr "length" "2")
   (set_attr "cc" "set_znv")])

(define_insn ""
  [(set (cc0)
	(and:SI (match_operand:SI 0 "register_operand" "r")
		(const_int -65536)))]
  ""
  "mov.w	%e0,%e0"
  [(set_attr "length" "2")
   (set_attr "cc" "set_znv")])

(define_insn "cmpqi"
  [(set (cc0)
	(compare:QI (match_operand:QI 0 "register_operand" "r")
		    (match_operand:QI 1 "nonmemory_operand" "rn")))]
  ""
  "cmp.b	%X1,%X0"
  [(set_attr "length" "2")
   (set_attr "cc" "compare")])

(define_expand "cmphi"
  [(set (cc0)
	(compare:HI (match_operand:HI 0 "register_operand" "")
		    (match_operand:HI 1 "nonmemory_operand" "")))]
  ""
  "
{
  /* Force operand1 into a register if we're compiling
     for the H8/300.  */
  if (GET_CODE (operands[1]) != REG && TARGET_H8300)
    operands[1] = force_reg (HImode, operands[1]);
}")

(define_insn ""
  [(set (cc0)
	(compare:HI (match_operand:HI 0 "register_operand" "r")
		    (match_operand:HI 1 "register_operand" "r")))]
  "TARGET_H8300"
  "cmp.w	%T1,%T0"
  [(set_attr "length" "2")
   (set_attr "cc" "compare")])

(define_insn ""
  [(set (cc0)
	(compare:HI (match_operand:HI 0 "register_operand" "r,r")
		    (match_operand:HI 1 "nonmemory_operand" "r,n")))]
  "TARGET_H8300H || TARGET_H8300S"
  "cmp.w	%T1,%T0"
  [(set_attr "length" "2,4")
   (set_attr "cc" "compare,compare")])

(define_insn "cmpsi"
  [(set (cc0)
	(compare:SI (match_operand:SI 0 "register_operand" "r,r")
		    (match_operand:SI 1 "nonmemory_operand" "r,i")))]
  "TARGET_H8300H || TARGET_H8300S"
  "cmp.l	%S1,%S0"
  [(set_attr "length" "2,6")
   (set_attr "cc" "compare,compare")])

;; ----------------------------------------------------------------------
;; ADD INSTRUCTIONS
;; ----------------------------------------------------------------------

(define_insn "addqi3"
  [(set (match_operand:QI 0 "register_operand" "=r")
	(plus:QI (match_operand:QI 1 "register_operand" "%0")
		 (match_operand:QI 2 "nonmemory_operand" "rn")))]
  ""
  "add.b	%X2,%X0"
  [(set_attr "length" "2")
   (set_attr "cc" "set_zn")])

(define_expand "addhi3"
  [(set (match_operand:HI 0 "register_operand" "")
	(plus:HI (match_operand:HI 1 "register_operand" "")
		 (match_operand:HI 2 "nonmemory_operand" "")))]
  ""
  "")

(define_insn "*addhi3_h8300"
  [(set (match_operand:HI 0 "register_operand" "=r,r,r,r,r")
	(plus:HI (match_operand:HI 1 "register_operand" "%0,0,0,0,0")
		 (match_operand:HI 2 "nonmemory_operand" "L,N,J,n,r")))]
  "TARGET_H8300"
  "@
   adds	%2,%T0
   subs	%G2,%T0
   add.b	%t2,%t0
   add.b	%s2,%s0\;addx	%t2,%t0
   add.w	%T2,%T0"
  [(set_attr "length" "2,2,2,4,2")
   (set_attr "cc" "none_0hit,none_0hit,clobber,clobber,set_zn")])

;; This splitter is very important to make the stack adjustment
;; interrupt-safe.  The combination of add.b and addx is unsafe!
;;
;; We apply this split after the peephole2 pass so that we won't end
;; up creating too many adds/subs when a scratch register is
;; available, which is actually a common case because stack unrolling
;; tends to happen immediately after a function call.

(define_split
  [(set (match_operand:HI 0 "stack_pointer_operand" "")
	(plus:HI (match_dup 0)
		 (match_operand 1 "const_int_gt_2_operand" "")))]
  "TARGET_H8300 && flow2_completed"
  [(const_int 0)]
  "split_adds_subs (HImode, operands); DONE;")

(define_peephole2
  [(match_scratch:HI 2 "r")
   (set (match_operand:HI 0 "stack_pointer_operand" "")
	(plus:HI (match_dup 0)
		 (match_operand:HI 1 "const_int_ge_8_operand" "")))]
  "TARGET_H8300"
  [(set (match_dup 2)
	(match_dup 1))
   (set (match_dup 0)
	(plus:HI (match_dup 0)
		 (match_dup 2)))]
  "")

(define_insn "*addhi3_h8300hs"
  [(set (match_operand:HI 0 "register_operand" "=r,r,r,r,r")
	(plus:HI (match_operand:HI 1 "register_operand" "%0,0,0,0,0")
		 (match_operand:HI 2 "nonmemory_operand" "L,N,J,n,r")))]
  "TARGET_H8300H || TARGET_H8300S"
  "@
   adds	%2,%S0
   subs	%G2,%S0
   add.b	%t2,%t0
   add.w	%T2,%T0
   add.w	%T2,%T0"
  [(set_attr "length" "2,2,2,4,2")
   (set_attr "cc" "none_0hit,none_0hit,clobber,set_zn,set_zn")])

(define_split
  [(set (match_operand:HI 0 "register_operand" "")
	(plus:HI (match_dup 0)
		 (match_operand:HI 1 "two_insn_adds_subs_operand" "")))]
  ""
  [(const_int 0)]
  "split_adds_subs (HImode, operands); DONE;")

(define_expand "addsi3"
  [(set (match_operand:SI 0 "register_operand" "")
	(plus:SI (match_operand:SI 1 "register_operand" "")
		 (match_operand:SI 2 "nonmemory_operand" "")))]
  ""
  "")

(define_insn "addsi_h8300"
  [(set (match_operand:SI 0 "register_operand" "=r,r,&r")
	(plus:SI (match_operand:SI 1 "register_operand" "%0,0,r")
		 (match_operand:SI 2 "nonmemory_operand" "n,r,r")))]
  "TARGET_H8300"
  "@
   add	%w2,%w0\;addx	%x2,%x0\;addx	%y2,%y0\;addx	%z2,%z0
   add.w	%f2,%f0\;addx	%y2,%y0\;addx	%z2,%z0
   mov.w	%f1,%f0\;mov.w	%e1,%e0\;add.w	%f2,%f0\;addx	%y2,%y0\;addx	%z2,%z0"
  [(set_attr "length" "8,6,10")
   (set_attr "cc" "clobber")])

(define_insn "addsi_h8300h"
  [(set (match_operand:SI 0 "register_operand" "=r,r,r,r")
	(plus:SI (match_operand:SI 1 "register_operand" "%0,0,0,0")
		 (match_operand:SI 2 "nonmemory_operand" "L,N,i,r")))]
  "TARGET_H8300H || TARGET_H8300S"
  "@
   adds	%2,%S0
   subs	%G2,%S0
   add.l	%S2,%S0
   add.l	%S2,%S0"
  [(set_attr "length" "2,2,6,2")
   (set_attr "cc" "none_0hit,none_0hit,set_zn,set_zn")])

(define_split
  [(set (match_operand:SI 0 "register_operand" "")
	(plus:SI (match_dup 0)
		 (match_operand:SI 1 "two_insn_adds_subs_operand" "")))]
  "TARGET_H8300H || TARGET_H8300S"
  [(const_int 0)]
  "split_adds_subs (SImode, operands); DONE;")

;; ----------------------------------------------------------------------
;; SUBTRACT INSTRUCTIONS
;; ----------------------------------------------------------------------

(define_insn "subqi3"
  [(set (match_operand:QI 0 "register_operand" "=r")
	(minus:QI (match_operand:QI 1 "register_operand" "0")
		  (match_operand:QI 2 "register_operand" "r")))]
  ""
  "sub.b	%X2,%X0"
  [(set_attr "length" "2")
   (set_attr "cc" "set_zn")])

(define_expand "subhi3"
  [(set (match_operand:HI 0 "register_operand" "")
	(minus:HI (match_operand:HI 1 "general_operand" "")
		  (match_operand:HI 2 "nonmemory_operand" "")))]
  ""
  "")

(define_insn ""
  [(set (match_operand:HI 0 "register_operand" "=r,&r")
	(minus:HI (match_operand:HI 1 "general_operand" "0,0")
		  (match_operand:HI 2 "nonmemory_operand" "r,n")))]
  "TARGET_H8300"
  "@
   sub.w	%T2,%T0
   add.b	%E2,%s0\;addx	%F2,%t0"
  [(set_attr "length" "2,4")
   (set_attr "cc" "set_zn,clobber")])

(define_insn ""
  [(set (match_operand:HI 0 "register_operand" "=r,&r")
	(minus:HI (match_operand:HI 1 "general_operand" "0,0")
		  (match_operand:HI 2 "nonmemory_operand" "r,n")))]
  "TARGET_H8300H || TARGET_H8300S"
  "@
   sub.w	%T2,%T0
   sub.w	%T2,%T0"
  [(set_attr "length" "2,4")
   (set_attr "cc" "set_zn,set_zn")])

(define_expand "subsi3"
  [(set (match_operand:SI 0 "register_operand" "")
	(minus:SI (match_operand:SI 1 "register_operand" "")
		  (match_operand:SI 2 "nonmemory_operand" "")))]
  ""
  "")

(define_insn "subsi3_h8300"
  [(set (match_operand:SI 0 "register_operand" "=r")
	(minus:SI (match_operand:SI 1 "register_operand" "0")
		  (match_operand:SI 2 "register_operand" "r")))]
  "TARGET_H8300"
  "sub.w	%f2,%f0\;subx	%y2,%y0\;subx	%z2,%z0"
  [(set_attr "length" "6")
   (set_attr "cc" "clobber")])

(define_insn "subsi3_h8300h"
  [(set (match_operand:SI 0 "register_operand" "=r,r")
	(minus:SI (match_operand:SI 1 "general_operand" "0,0")
		  (match_operand:SI 2 "nonmemory_operand" "r,i")))]
  "TARGET_H8300H || TARGET_H8300S"
  "@
   sub.l	%S2,%S0
   sub.l	%S2,%S0"
  [(set_attr "length" "2,6")
   (set_attr "cc" "set_zn,set_zn")])

;; ----------------------------------------------------------------------
;; MULTIPLY INSTRUCTIONS
;; ----------------------------------------------------------------------

;; Note that the H8/300 can only handle umulqihi3.

(define_insn "mulqihi3"
  [(set (match_operand:HI 0 "register_operand" "=r")
	(mult:HI (sign_extend:HI (match_operand:QI 1 "register_operand" "%0"))
		 (sign_extend:HI (match_operand:QI 2 "register_operand" "r"))))]
  "TARGET_H8300H || TARGET_H8300S"
  "mulxs.b	%X2,%T0"
  [(set_attr "length" "4")
   (set_attr "cc" "set_zn")])

(define_insn "mulhisi3"
  [(set (match_operand:SI 0 "register_operand" "=r")
	(mult:SI (sign_extend:SI (match_operand:HI 1 "register_operand" "%0"))
		 (sign_extend:SI (match_operand:HI 2 "register_operand" "r"))))]
  "TARGET_H8300H || TARGET_H8300S"
  "mulxs.w	%T2,%S0"
  [(set_attr "length" "4")
   (set_attr "cc" "set_zn")])

(define_insn "umulqihi3"
  [(set (match_operand:HI 0 "register_operand" "=r")
	(mult:HI (zero_extend:HI (match_operand:QI 1 "register_operand" "%0"))
		 (zero_extend:HI (match_operand:QI 2 "register_operand" "r"))))]
  ""
  "mulxu	%X2,%T0"
  [(set_attr "length" "2")
   (set_attr "cc" "none_0hit")])

(define_insn "umulhisi3"
  [(set (match_operand:SI 0 "register_operand" "=r")
	(mult:SI (zero_extend:SI (match_operand:HI 1 "register_operand" "%0"))
		 (zero_extend:SI (match_operand:HI 2 "register_operand" "r"))))]
  "TARGET_H8300H || TARGET_H8300S"
  "mulxu.w	%T2,%S0"
  [(set_attr "length" "2")
   (set_attr "cc" "none_0hit")])

;; This is a "bridge" instruction.  Combine can't cram enough insns
;; together to crate a MAC instruction directly, but it can create
;; this instruction, which then allows combine to create the real
;; MAC insn.
;;
;; Unfortunately, if combine doesn't create a MAC instruction, this
;; insn must generate reasonably correct code.  Egad.
(define_insn ""
  [(set (match_operand:SI 0 "register_operand" "=a")
	(mult:SI
	  (sign_extend:SI
	    (mem:HI (post_inc:SI (match_operand:SI 1 "register_operand" "r"))))
	  (sign_extend:SI
	    (mem:HI (post_inc:SI (match_operand:SI 2 "register_operand" "r"))))))]
  "TARGET_MAC"
  "clrmac\;mac	@%2+,@%1+"
  [(set_attr "length" "6")
   (set_attr "cc" "none_0hit")])

(define_insn ""
  [(set (match_operand:SI 0 "register_operand" "=a")
	(plus:SI (mult:SI
	  (sign_extend:SI (mem:HI
	    (post_inc:SI (match_operand:SI 1 "register_operand" "r"))))
	  (sign_extend:SI (mem:HI
	    (post_inc:SI (match_operand:SI 2 "register_operand" "r")))))
	      (match_operand:SI 3 "register_operand" "0")))]
  "TARGET_MAC"
  "mac	@%2+,@%1+"
  [(set_attr "length" "4")
   (set_attr "cc" "none_0hit")])

;; ----------------------------------------------------------------------
;; DIVIDE/MOD INSTRUCTIONS
;; ----------------------------------------------------------------------

(define_insn "udivmodqi4"
  [(set (match_operand:QI 0 "register_operand" "=r")
	(truncate:QI
	  (udiv:HI
	    (match_operand:HI 1 "register_operand" "0")
	    (zero_extend:HI (match_operand:QI 2 "register_operand" "r")))))
   (set (match_operand:QI 3 "register_operand" "=r")
	(truncate:QI
	  (umod:HI
	    (match_dup 1)
	    (zero_extend:HI (match_dup 2)))))]
  ""
  "*
{
  if (find_reg_note (insn, REG_UNUSED, operands[3]))
    return \"divxu.b\\t%X2,%T0\";
  else
    return \"divxu.b\\t%X2,%T0\;mov.b\\t%t0,%s3\";
}"
  [(set_attr "length" "4")
   (set_attr "cc" "clobber")])

(define_insn "divmodqi4"
  [(set (match_operand:QI 0 "register_operand" "=r")
	(truncate:QI
	  (div:HI
	    (match_operand:HI 1 "register_operand" "0")
	    (sign_extend:HI (match_operand:QI 2 "register_operand" "r")))))
   (set (match_operand:QI 3 "register_operand" "=r")
	(truncate:QI
	  (mod:HI
	    (match_dup 1)
	    (sign_extend:HI (match_dup 2)))))]
  "TARGET_H8300H || TARGET_H8300S"
  "*
{
  if (find_reg_note (insn, REG_UNUSED, operands[3]))
    return \"divxs.b\\t%X2,%T0\";
  else
    return \"divxs.b\\t%X2,%T0\;mov.b\\t%t0,%s3\";
}"
  [(set_attr "length" "6")
   (set_attr "cc" "clobber")])

(define_insn "udivmodhi4"
  [(set (match_operand:HI 0 "register_operand" "=r")
	(truncate:HI
	  (udiv:SI
	    (match_operand:SI 1 "register_operand" "0")
	    (zero_extend:SI (match_operand:HI 2 "register_operand" "r")))))
   (set (match_operand:HI 3 "register_operand" "=r")
	(truncate:HI
	  (umod:SI
	    (match_dup 1)
	    (zero_extend:SI (match_dup 2)))))]
  "TARGET_H8300H || TARGET_H8300S"
  "*
{
  if (find_reg_note (insn, REG_UNUSED, operands[3]))
    return \"divxu.w\\t%T2,%S0\";
  else
    return \"divxu.w\\t%T2,%S0\;mov.w\\t%e0,%f3\";
}"
  [(set_attr "length" "4")
   (set_attr "cc" "clobber")])

(define_insn "divmodhi4"
  [(set (match_operand:HI 0 "register_operand" "=r")
	(truncate:HI
	  (div:SI
	    (match_operand:SI 1 "register_operand" "0")
	    (sign_extend:SI (match_operand:HI 2 "register_operand" "r")))))
   (set (match_operand:HI 3 "register_operand" "=r")
	(truncate:HI
	  (mod:SI
	    (match_dup 1)
	    (sign_extend:SI (match_dup 2)))))]
  "TARGET_H8300H || TARGET_H8300S"
  "*
{
  if (find_reg_note (insn, REG_UNUSED, operands[3]))
    return \"divxs.w\\t%T2,%S0\";
  else
    return \"divxs.w\\t%T2,%S0\;mov.w\\t%e0,%f3\";
}"
  [(set_attr "length" "6")
   (set_attr "cc" "clobber")])

;; ----------------------------------------------------------------------
;; AND INSTRUCTIONS
;; ----------------------------------------------------------------------

(define_insn ""
  [(set (match_operand:QI 0 "bit_operand" "=r,U")
	(and:QI (match_operand:QI 1 "bit_operand" "%0,0")
		(match_operand:QI 2 "nonmemory_operand" "rn,n")))]
  "register_operand (operands[0], QImode)
   || single_zero_operand (operands[2], QImode)"
  "@
   and	%X2,%X0
   bclr	%W2,%R0"
  [(set_attr "length" "2,8")
   (set_attr "adjust_length" "no")
   (set_attr "cc" "set_znv,none_0hit")])

(define_expand "andqi3"
  [(set (match_operand:QI 0 "bit_operand" "")
	(and:QI (match_operand:QI 1 "bit_operand" "")
		(match_operand:QI 2 "nonmemory_operand" "")))]
  ""
  "
{
  if (fix_bit_operand (operands, 0, AND))
    DONE;
}")

(define_expand "andhi3"
  [(set (match_operand:HI 0 "register_operand" "")
	(and:HI (match_operand:HI 1 "register_operand" "")
		(match_operand:HI 2 "nonmemory_operand" "")))]
  ""
  "")

(define_insn "*andorqi3"
  [(set (match_operand:QI 0 "register_operand" "=r")
	(ior:QI (and:QI (match_operand:QI 2 "register_operand" "r")
			(match_operand:QI 3 "single_one_operand" "n"))
		(match_operand:QI 1 "register_operand" "0")))]
  ""
  "bld\\t%V3,%X2\;bor\\t%V3,%X0\;bst\\t%V3,%X0"
  [(set_attr "length" "6")
   (set_attr "cc" "clobber")])

(define_insn "*andorhi3"
  [(set (match_operand:HI 0 "register_operand" "=r")
	(ior:HI (and:HI (match_operand:HI 2 "register_operand" "r")
			(match_operand:HI 3 "single_one_operand" "n"))
		(match_operand:HI 1 "register_operand" "0")))]
  ""
  "*
{
  operands[3] = GEN_INT (INTVAL (operands[3]) & 0xffff);
  if (INTVAL (operands[3]) > 128)
    {
      operands[3] = GEN_INT (INTVAL (operands[3]) >> 8);
      return \"bld\\t%V3,%t2\;bor\\t%V3,%t0\;bst\\t%V3,%t0\";
    }
  return \"bld\\t%V3,%s2\;bor\\t%V3,%s0\;bst\\t%V3,%s0\";
}"
  [(set_attr "length" "6")
   (set_attr "cc" "clobber")])

(define_insn "*andorsi3"
  [(set (match_operand:SI 0 "register_operand" "=r")
	(ior:SI (and:SI (match_operand:SI 2 "register_operand" "r")
			(match_operand:SI 3 "single_one_operand" "n"))
		(match_operand:SI 1 "register_operand" "0")))]
  "(INTVAL (operands[3]) & 0xffff) != 0"
  "*
{
  operands[3] = GEN_INT (INTVAL (operands[3]) & 0xffff);
  if (INTVAL (operands[3]) > 128)
    {
      operands[3] = GEN_INT (INTVAL (operands[3]) >> 8);
      return \"bld\\t%V3,%x2\;bor\\t%V3,%x0\;bst\\t%V3,%x0\";
    }
  return \"bld\\t%V3,%w2\;bor\\t%V3,%w0\;bst\\t%V3,%w0\";
}"
  [(set_attr "length" "6")
   (set_attr "cc" "clobber")])

(define_insn "*andorsi3_shift_8"
  [(set (match_operand:SI 0 "register_operand" "=r")
	(ior:SI (and:SI (ashift:SI (match_operand:SI 2 "register_operand" "r")
				   (const_int 8))
			(const_int 65280))
		(match_operand:SI 1 "register_operand" "0")))]
  ""
  "or.b\\t%w2,%x0"
  [(set_attr "length" "2")
   (set_attr "cc" "clobber")])

(define_expand "andsi3"
  [(set (match_operand:SI 0 "register_operand" "")
	(and:SI (match_operand:SI 1 "register_operand" "")
		(match_operand:SI 2 "nonmemory_operand" "")))]
  ""
  "")

;; ----------------------------------------------------------------------
;; OR INSTRUCTIONS
;; ----------------------------------------------------------------------

(define_insn ""
  [(set (match_operand:QI 0 "bit_operand" "=r,U")
	(ior:QI (match_operand:QI 1 "bit_operand" "%0,0")
		(match_operand:QI 2 "nonmemory_operand" "rn,n")))]
  "register_operand (operands[0], QImode)
   || single_one_operand (operands[2], QImode)"
  "@
   or\\t%X2,%X0
   bset\\t%V2,%R0"
  [(set_attr "length" "2,8")
   (set_attr "adjust_length" "no")
   (set_attr "cc" "set_znv,none_0hit")])

(define_expand "iorqi3"
  [(set (match_operand:QI 0 "bit_operand" "")
	(ior:QI (match_operand:QI 1 "bit_operand" "")
		(match_operand:QI 2 "nonmemory_operand" "")))]
  ""
  "
{
  if (fix_bit_operand (operands, 1, IOR))
    DONE;
}")

(define_expand "iorhi3"
  [(set (match_operand:HI 0 "register_operand" "")
	(ior:HI (match_operand:HI 1 "register_operand" "")
		(match_operand:HI 2 "nonmemory_operand" "")))]
  ""
  "")

(define_expand "iorsi3"
  [(set (match_operand:SI 0 "register_operand" "")
	(ior:SI (match_operand:SI 1 "register_operand" "")
		(match_operand:SI 2 "nonmemory_operand" "")))]
  ""
  "")

;; ----------------------------------------------------------------------
;; XOR INSTRUCTIONS
;; ----------------------------------------------------------------------

(define_insn ""
  [(set (match_operand:QI 0 "bit_operand" "=r,U")
	(xor:QI (match_operand:QI 1 "bit_operand" "%0,0")
		(match_operand:QI 2 "nonmemory_operand" "rn,n")))]
  "register_operand (operands[0], QImode)
   || single_one_operand (operands[2], QImode)"
  "@
   xor\\t%X2,%X0
   bnot\\t%V2,%R0"
  [(set_attr "length" "2,8")
   (set_attr "adjust_length" "no")
   (set_attr "cc" "set_znv,none_0hit")])

(define_expand "xorqi3"
  [(set (match_operand:QI 0 "bit_operand" "")
	(xor:QI (match_operand:QI 1 "bit_operand" "")
		(match_operand:QI 2 "nonmemory_operand" "")))]
  ""
  "
{
  if (fix_bit_operand (operands, 1, XOR))
    DONE;
}")

(define_expand "xorhi3"
  [(set (match_operand:HI 0 "register_operand" "")
	(xor:HI (match_operand:HI 1 "register_operand" "")
		(match_operand:HI 2 "nonmemory_operand" "")))]
  ""
  "")

(define_expand "xorsi3"
  [(set (match_operand:SI 0 "register_operand" "")
	(xor:SI (match_operand:SI 1 "register_operand" "")
		(match_operand:SI 2 "nonmemory_operand" "")))]
  ""
  "")

;; ----------------------------------------------------------------------
;; {AND,IOR,XOR}{HI3,SI3} PATTERNS
;; ----------------------------------------------------------------------

(define_insn ""
  [(set (match_operand:HI 0 "register_operand" "=r")
	(match_operator:HI 3 "bit_operator"
	  [(match_operand:HI 1 "register_operand" "%0")
	   (match_operand:HI 2 "nonmemory_operand" "rn")]))]
  ""
  "* return output_logical_op (HImode, operands);"
  [(set (attr "length")
	(symbol_ref "compute_logical_op_length (HImode, operands)"))
   (set (attr "cc")
	(symbol_ref "compute_logical_op_cc (HImode, operands)"))])

(define_insn ""
  [(set (match_operand:SI 0 "register_operand" "=r")
	(match_operator:SI 3 "bit_operator"
	  [(match_operand:SI 1 "register_operand" "%0")
	   (match_operand:SI 2 "nonmemory_operand" "rn")]))]
  ""
  "* return output_logical_op (SImode, operands);"
  [(set (attr "length")
	(symbol_ref "compute_logical_op_length (SImode, operands)"))
   (set (attr "cc")
	(symbol_ref "compute_logical_op_cc (SImode, operands)"))])

;; ----------------------------------------------------------------------
;; NEGATION INSTRUCTIONS
;; ----------------------------------------------------------------------

(define_insn "negqi2"
  [(set (match_operand:QI 0 "register_operand" "=r")
	(neg:QI (match_operand:QI 1 "register_operand" "0")))]
  ""
  "neg	%X0"
  [(set_attr "length" "2")
   (set_attr "cc" "set_zn")])

(define_expand "neghi2"
  [(set (match_operand:HI 0 "register_operand" "")
	(neg:HI (match_operand:HI 1 "register_operand" "")))]
  ""
  "
{
  if (TARGET_H8300)
    {
      emit_insn (gen_neghi2_h8300 (operands[0], operands[1]));
      DONE;
    }
}")

(define_expand "neghi2_h8300"
  [(set (match_dup 2)
	(not:HI (match_operand:HI 1 "register_operand" "")))
   (set (match_dup 2) (plus:HI (match_dup 2) (const_int 1)))
   (set (match_operand:HI 0 "register_operand" "")
	(match_dup 2))]
  ""
  "operands[2] = gen_reg_rtx (HImode);")

(define_insn "neghi2_h8300h"
  [(set (match_operand:HI 0 "register_operand" "=r")
	(neg:HI (match_operand:HI 1 "register_operand" "0")))]
  "TARGET_H8300H || TARGET_H8300S"
  "neg	%T0"
  [(set_attr "length" "2")
   (set_attr "cc" "set_zn")])

(define_expand "negsi2"
  [(set (match_operand:SI 0 "register_operand" "")
	(neg:SI (match_operand:SI 1 "register_operand" "")))]
  ""
  "
{
  if (TARGET_H8300)
    {
      emit_insn (gen_negsi2_h8300 (operands[0], operands[1]));
      DONE;
    }
}")

(define_expand "negsi2_h8300"
  [(set (match_dup 2)
	(not:SI (match_operand:SI 1 "register_operand" "")))
   (set (match_dup 2) (plus:SI (match_dup 2) (const_int 1)))
   (set (match_operand:SI 0 "register_operand" "")
	(match_dup 2))]
  ""
  "operands[2] = gen_reg_rtx (SImode);")

(define_insn "negsi2_h8300h"
  [(set (match_operand:SI 0 "register_operand" "=r")
	(neg:SI (match_operand:SI 1 "register_operand" "0")))]
  "TARGET_H8300H || TARGET_H8300S"
  "neg	%S0"
  [(set_attr "length" "2")
   (set_attr "cc" "set_zn")])

;; ----------------------------------------------------------------------
;; NOT INSTRUCTIONS
;; ----------------------------------------------------------------------

(define_insn "one_cmplqi2"
  [(set (match_operand:QI 0 "register_operand" "=r")
	(not:QI (match_operand:QI 1 "register_operand" "0")))]
  ""
  "not	%X0"
  [(set_attr "length" "2")
   (set_attr "cc" "set_znv")])

(define_expand "one_cmplhi2"
  [(set (match_operand:HI 0 "register_operand" "=r")
	(not:HI (match_operand:HI 1 "register_operand" "0")))]
  ""
  "")

(define_insn ""
  [(set (match_operand:HI 0 "register_operand" "=r")
	(not:HI (match_operand:HI 1 "register_operand" "0")))]
  "TARGET_H8300"
  "not	%s0\;not	%t0"
  [(set_attr "cc" "clobber")
   (set_attr "length" "4")])

(define_insn ""
  [(set (match_operand:HI 0 "register_operand" "=r")
	(not:HI (match_operand:HI 1 "register_operand" "0")))]
  "TARGET_H8300H || TARGET_H8300S"
  "not	%T0"
  [(set_attr "cc" "set_znv")
   (set_attr "length" "2")])

(define_expand "one_cmplsi2"
  [(set (match_operand:SI 0 "register_operand" "=r")
	(not:SI (match_operand:SI 1 "register_operand" "0")))]
  ""
  "")

(define_insn ""
  [(set (match_operand:SI 0 "register_operand" "=r")
	(not:SI (match_operand:SI 1 "register_operand" "0")))]
  "TARGET_H8300"
  "not	%w0\;not	%x0\;not	%y0\;not	%z0"
  [(set_attr "cc" "clobber")
   (set_attr "length" "8")])

(define_insn ""
  [(set (match_operand:SI 0 "register_operand" "=r")
	(not:SI (match_operand:SI 1 "register_operand" "0")))]
  "TARGET_H8300H || TARGET_H8300S"
  "not	%S0"
  [(set_attr "cc" "set_znv")
   (set_attr "length" "2")])

;; ----------------------------------------------------------------------
;; JUMP INSTRUCTIONS
;; ----------------------------------------------------------------------

;; Conditional jump instructions

(define_expand "ble"
  [(set (pc)
	(if_then_else (le (cc0)
			  (const_int 0))
		      (label_ref (match_operand 0 "" ""))
		      (pc)))]
  ""
  "")

(define_expand "bleu"
  [(set (pc)
	(if_then_else (leu (cc0)
			   (const_int 0))
		      (label_ref (match_operand 0 "" ""))
		      (pc)))]
  ""
  "")

(define_expand "bge"
  [(set (pc)
	(if_then_else (ge (cc0)
			  (const_int 0))
		      (label_ref (match_operand 0 "" ""))
		      (pc)))]
  ""
  "")

(define_expand "bgeu"
  [(set (pc)
	(if_then_else (geu (cc0)
			   (const_int 0))
		      (label_ref (match_operand 0 "" ""))
		      (pc)))]
  ""
  "")

(define_expand "blt"
  [(set (pc)
	(if_then_else (lt (cc0)
			  (const_int 0))
		      (label_ref (match_operand 0 "" ""))
		      (pc)))]
  ""
  "")

(define_expand "bltu"
  [(set (pc)
	(if_then_else (ltu (cc0)
			   (const_int 0))
		      (label_ref (match_operand 0 "" ""))
		      (pc)))]
  ""
  "")

(define_expand "bgt"
  [(set (pc)
	(if_then_else (gt (cc0)
			  (const_int 0))
		      (label_ref (match_operand 0 "" ""))
		      (pc)))]
  ""
  "")

(define_expand "bgtu"
  [(set (pc)
	(if_then_else (gtu (cc0)
			   (const_int 0))
		      (label_ref (match_operand 0 "" ""))
		      (pc)))]
  ""
  "")

(define_expand "beq"
  [(set (pc)
	(if_then_else (eq (cc0)
			  (const_int 0))
		      (label_ref (match_operand 0 "" ""))
		      (pc)))]
  ""
  "")

(define_expand "bne"
  [(set (pc)
	(if_then_else (ne (cc0)
			  (const_int 0))
		      (label_ref (match_operand 0 "" ""))
		      (pc)))]
  ""
  "")

(define_insn "branch_true"
  [(set (pc)
	(if_then_else (match_operator 1 "comparison_operator"
				      [(cc0) (const_int 0)])
		      (label_ref (match_operand 0 "" ""))
		      (pc)))]
  ""
  "*
{
  if ((cc_status.flags & CC_OVERFLOW_UNUSABLE) != 0
      && (GET_CODE (operands[1]) == GT
	  || GET_CODE (operands[1]) == GE
	  || GET_CODE (operands[1]) == LE
	  || GET_CODE (operands[1]) == LT))
    {
      cc_status.flags &= ~CC_OVERFLOW_UNUSABLE;
      return 0;
    }

  if (get_attr_length (insn) == 2)
    return \"b%j1	%l0\";
  else if (get_attr_length (insn) == 4)
    return \"b%j1	%l0:16\";
  else
    return \"b%k1	.Lh8BR%=\;jmp	@%l0\\n.Lh8BR%=:\";
}"
 [(set_attr "type" "branch")
   (set_attr "cc" "none")])

(define_insn "branch_false"
  [(set (pc)
	(if_then_else (match_operator 1 "comparison_operator"
				      [(cc0) (const_int 0)])
		      (pc)
		      (label_ref (match_operand 0 "" ""))))]
  ""
  "*
{
  if ((cc_status.flags & CC_OVERFLOW_UNUSABLE) != 0
      && (GET_CODE (operands[1]) == GT
	  || GET_CODE (operands[1]) == GE
	  || GET_CODE (operands[1]) == LE
	  || GET_CODE (operands[1]) == LT))
    {
      cc_status.flags &= ~CC_OVERFLOW_UNUSABLE;
      return 0;
    }

  if (get_attr_length (insn) == 2)
    return \"b%k1	%l0\";
  else if (get_attr_length (insn) == 4)
    return \"b%k1	%l0:16\";
  else
    return \"b%j1	.Lh8BR%=\;jmp	@%l0\\n.Lh8BR%=:\";
}"
  [(set_attr "type" "branch")
   (set_attr "cc" "none")])

;; Unconditional and other jump instructions.

(define_insn "jump"
  [(set (pc)
	(label_ref (match_operand 0 "" "")))]
  ""
  "*
{
  if (get_attr_length (insn) == 2)
    return \"bra	%l0\";
  else if (get_attr_length (insn) == 4)
    return \"bra	%l0:16\";
  else
    return \"jmp	@%l0\";
}"
  [(set_attr "type" "branch")
   (set_attr "cc" "none")])

;; This is a define expand, because pointers may be either 16 or 32 bits.

(define_expand "tablejump"
  [(parallel [(set (pc) (match_operand 0 "register_operand" ""))
	      (use (label_ref (match_operand 1 "" "")))])]
  ""
  "")

(define_insn "tablejump_h8300"
  [(set (pc) (match_operand:HI 0 "register_operand" "r"))
   (use (label_ref (match_operand 1 "" "")))]
  "TARGET_H8300"
  "jmp	@%0"
  [(set_attr "cc" "none")
   (set_attr "length" "2")])

(define_insn "tablejump_h8300h"
  [(set (pc) (match_operand:SI 0 "register_operand" "r"))
   (use (label_ref (match_operand 1 "" "")))]
  "TARGET_H8300H || TARGET_H8300S"
  "jmp	@%0"
  [(set_attr "cc" "none")
   (set_attr "length" "2")])

(define_insn "tablejump_normal_mode"
   [(set (pc) (match_operand:HI 0 "register_operand" "r"))
    (use (label_ref (match_operand 1 "" "")))]
   "(TARGET_H8300H || TARGET_H8300S) && TARGET_NORMAL_MODE"
   "jmp @%S0"
   [(set_attr "cc" "none")
    (set_attr "length" "2")])

;; This is a define expand, because pointers may be either 16 or 32 bits.

(define_expand "indirect_jump"
  [(set (pc) (match_operand 0 "jump_address_operand" ""))]
  ""
  "")

(define_insn "indirect_jump_h8300"
  [(set (pc) (match_operand:HI 0 "jump_address_operand" "Vr"))]
  "TARGET_H8300"
  "jmp	@%0"
  [(set_attr "cc" "none")
   (set_attr "length" "2")])

(define_insn "indirect_jump_h8300h"
  [(set (pc) (match_operand:SI 0 "jump_address_operand" "Vr"))]
  "TARGET_H8300H || TARGET_H8300S"
  "jmp @%0"
  [(set_attr "cc" "none")
   (set_attr "length" "2")])

(define_insn "indirect_jump_normal_mode"
  [(set (pc) (match_operand:HI 0 "jump_address_operand" "Vr"))]
  "(TARGET_H8300H || TARGET_H8300S) && TARGET_NORMAL_MODE"
  "jmp @%S0"
  [(set_attr "cc" "none")
   (set_attr "length" "2")])

;; Call subroutine with no return value.

;; ??? Even though we use HImode here, this works on the H8/300H and H8S.

(define_insn "call"
  [(call (match_operand:QI 0 "call_insn_operand" "or")
	 (match_operand:HI 1 "general_operand" "g"))]
  ""
  "*
{
  if (GET_CODE (XEXP (operands[0], 0)) == SYMBOL_REF
      && SYMBOL_REF_FLAG (XEXP (operands[0], 0)))
    return \"jsr\\t@%0:8\";
  else
    return \"jsr\\t%0\";
}"
  [(set_attr "cc" "clobber")
   (set (attr "length")
	(if_then_else (match_operand:QI 0 "small_call_insn_operand" "")
		      (const_int 4)
		      (const_int 8)))])

;; Call subroutine, returning value in operand 0
;; (which must be a hard register).

;; ??? Even though we use HImode here, this works on the H8/300H and H8S.

(define_insn "call_value"
  [(set (match_operand 0 "" "=r")
	(call (match_operand:QI 1 "call_insn_operand" "or")
	      (match_operand:HI 2 "general_operand" "g")))]
  ""
  "*
{
  if (GET_CODE (XEXP (operands[1], 0)) == SYMBOL_REF
      && SYMBOL_REF_FLAG (XEXP (operands[1], 0)))
    return \"jsr\\t@%1:8\";
  else
    return \"jsr\\t%1\";
}"
  [(set_attr "cc" "clobber")
   (set (attr "length")
	(if_then_else (match_operand:QI 0 "small_call_insn_operand" "")
		      (const_int 4)
		      (const_int 8)))])

(define_insn "nop"
  [(const_int 0)]
  ""
  "nop"
  [(set_attr "cc" "none")
   (set_attr "length" "2")])

;; ----------------------------------------------------------------------
;; PROLOGUE/EPILOGUE-RELATED INSTRUCTIONS
;; ----------------------------------------------------------------------

(define_insn "*stm_h8300s_2"
  [(parallel
     [(set (reg:SI SP_REG)
	   (plus:SI (reg:SI SP_REG) (const_int -8)))
      (set (mem:SI (plus:SI (reg:SI SP_REG) (const_int -4)))
	   (match_operand:SI 0 "register_operand" ""))
      (set (mem:SI (plus:SI (reg:SI SP_REG) (const_int -8)))
	   (match_operand:SI 1 "register_operand" ""))])]
  "TARGET_H8300S
   && ((REGNO (operands[0]) == 0 && REGNO (operands[1]) == 1)
       || (REGNO (operands[0]) == 2 && REGNO (operands[1]) == 3)
       || (REGNO (operands[0]) == 4 && REGNO (operands[1]) == 5))"
  "stm.l\\t%S0-%S1,@-er7"
  [(set_attr "cc" "none")
   (set_attr "length" "4")])

(define_insn "*stm_h8300s_3"
  [(parallel
     [(set (reg:SI SP_REG)
	   (plus:SI (reg:SI SP_REG) (const_int -12)))
      (set (mem:SI (plus:SI (reg:SI SP_REG) (const_int -4)))
	   (match_operand:SI 0 "register_operand" ""))
      (set (mem:SI (plus:SI (reg:SI SP_REG) (const_int -8)))
	   (match_operand:SI 1 "register_operand" ""))
      (set (mem:SI (plus:SI (reg:SI SP_REG) (const_int -12)))
	   (match_operand:SI 2 "register_operand" ""))])]
  "TARGET_H8300S
   && ((REGNO (operands[0]) == 0
	&& REGNO (operands[1]) == 1
	&& REGNO (operands[2]) == 2)
       || (REGNO (operands[0]) == 4
	   && REGNO (operands[1]) == 5
	   && REGNO (operands[2]) == 6))"
  "stm.l\\t%S0-%S2,@-er7"
  [(set_attr "cc" "none")
   (set_attr "length" "4")])

(define_insn "*stm_h8300s_4"
  [(parallel
     [(set (reg:SI SP_REG)
	   (plus:SI (reg:SI SP_REG) (const_int -16)))
      (set (mem:SI (plus:SI (reg:SI SP_REG) (const_int -4)))
	   (match_operand:SI 0 "register_operand" ""))
      (set (mem:SI (plus:SI (reg:SI SP_REG) (const_int -8)))
	   (match_operand:SI 1 "register_operand" ""))
      (set (mem:SI (plus:SI (reg:SI SP_REG) (const_int -12)))
	   (match_operand:SI 2 "register_operand" ""))
      (set (mem:SI (plus:SI (reg:SI SP_REG) (const_int -16)))
	   (match_operand:SI 3 "register_operand" ""))])]
  "TARGET_H8300S
   && REGNO (operands[0]) == 0
   && REGNO (operands[1]) == 1
   && REGNO (operands[2]) == 2
   && REGNO (operands[3]) == 3"
  "stm.l\\t%S0-%S3,@-er7"
  [(set_attr "cc" "none")
   (set_attr "length" "4")])

;; ----------------------------------------------------------------------
;; EXTEND INSTRUCTIONS
;; ----------------------------------------------------------------------

(define_expand "zero_extendqihi2"
  [(set (match_operand:HI 0 "register_operand" "")
	(zero_extend:HI (match_operand:QI 1 "general_operand_src" "")))]
  ""
  "")

(define_insn ""
  [(set (match_operand:HI 0 "register_operand" "=r,r")
	(zero_extend:HI (match_operand:QI 1 "general_operand_src" "0,g>")))]
  "TARGET_H8300"
  "@
  mov.b	#0,%t0
  mov.b	%R1,%s0\;mov.b	#0,%t0"
  [(set_attr "length" "2,10")
   (set_attr "cc" "clobber,clobber")])

(define_insn ""
  [(set (match_operand:HI 0 "register_operand" "=r,r")
	(zero_extend:HI (match_operand:QI 1 "general_operand_src" "0,g>")))]
  "TARGET_H8300H || TARGET_H8300S"
  "@
  extu.w	%T0
  mov.b	%R1,%s0\;extu.w	%T0"
  [(set_attr "length" "2,10")
   (set_attr "cc" "set_znv,set_znv")])

;; The compiler can synthesize a H8/300H variant of this which is
;; just as efficient as one that we'd create
(define_insn "zero_extendqisi2"
  [(set (match_operand:SI 0 "register_operand" "=r,r")
	(zero_extend:SI (match_operand:QI 1 "general_operand_src" "0,g>")))]
  "TARGET_H8300"
  "@
  mov.b	#0,%x0\;sub.w	%e0,%e0
  mov.b	%R1,%w0\;mov.b	#0,%x0\;sub.w	%e0,%e0"
  [(set_attr "length" "4,8")
   (set_attr "cc" "clobber,clobber")])

(define_expand "zero_extendhisi2"
  [(set (match_operand:SI 0 "register_operand" "")
	(zero_extend:SI (match_operand:HI 1 "register_operand" "")))]
  ""
  "")

;; %e prints the high part of a CONST_INT, not the low part.  Arggh.
(define_insn "*zero_extendhisi2_h8300"
  [(set (match_operand:SI 0 "register_operand" "=r,r,r")
	(zero_extend:SI (match_operand:HI 1 "general_operand_src" "0,i,g>")))]
  "TARGET_H8300"
  "@
  sub.w	%e0,%e0
  mov.w	%f1,%f0\;sub.w	%e0,%e0
  mov.w	%e1,%f0\;sub.w	%e0,%e0"
  [(set_attr "length" "2,4,6")
   (set_attr "cc" "clobber,clobber,clobber")])

(define_insn ""
  [(set (match_operand:SI 0 "register_operand" "=r")
	(zero_extend:SI (match_operand:HI 1 "register_operand" "0")))]
  "TARGET_H8300H || TARGET_H8300S"
  "extu.l	%S0"
  [(set_attr "length" "2")
   (set_attr "cc" "set_znv")])

(define_expand "extendqihi2"
  [(set (match_operand:HI 0 "register_operand" "")
	(sign_extend:HI (match_operand:QI 1 "register_operand" "")))]
  ""
  "")

(define_insn ""
  [(set (match_operand:HI 0 "register_operand" "=r,r")
	(sign_extend:HI (match_operand:QI 1 "general_operand_src" "0,g>")))]
  "TARGET_H8300"
  "@
  bld	#7,%s0\;subx	%t0,%t0
  mov.b	%R1,%s0\;bld	#7,%s0\;subx	%t0,%t0"
  [(set_attr "length" "4,8")
   (set_attr "cc" "clobber,clobber")])

(define_insn ""
  [(set (match_operand:HI 0 "register_operand" "=r")
	(sign_extend:HI (match_operand:QI 1 "register_operand" "0")))]
  "TARGET_H8300H || TARGET_H8300S"
  "exts.w	%T0"
  [(set_attr "length" "2")
   (set_attr "cc" "set_znv")])

;; The compiler can synthesize a H8/300H variant of this which is
;; just as efficient as one that we'd create
(define_insn "extendqisi2"
  [(set (match_operand:SI 0 "register_operand" "=r,r")
	(sign_extend:SI (match_operand:QI 1 "general_operand_src" "0,g>")))]
  "TARGET_H8300"
  "@
  bld	#7,%w0\;subx	%x0,%x0\;subx	%y0,%y0\;subx	%z0,%z0
  mov.b	%R1,%w0\;bld	#7,%w0\;subx	%x0,%x0\;subx	%y0,%y0\;subx	%z0,%z0"
  [(set_attr "length" "8,12")
   (set_attr "cc" "clobber,clobber")])

(define_expand "extendhisi2"
  [(set (match_operand:SI 0 "register_operand" "")
	(sign_extend:SI (match_operand:HI 1 "register_operand" "")))]
  ""
  "")

(define_insn "*extendhisi2_h8300"
  [(set (match_operand:SI 0 "register_operand" "=r,r")
	(sign_extend:SI (match_operand:HI 1 "general_operand_src" "0,g>")))]
  "TARGET_H8300"
  "@
  bld	#7,%x0\;subx	%y0,%y0\;subx	%z0,%z0
  mov.w	%T1,%f0\;bld	#7,%x0\;subx	%y0,%y0\;subx	%z0,%z0"
  [(set_attr "length" "6,10")
   (set_attr "cc" "clobber,clobber")])

(define_insn ""
  [(set (match_operand:SI 0 "register_operand" "=r")
	(sign_extend:SI (match_operand:HI 1 "register_operand" "0")))]
  "TARGET_H8300H || TARGET_H8300S"
  "exts.l	%S0"
  [(set_attr "length" "2")
   (set_attr "cc" "set_znv")])

;; ----------------------------------------------------------------------
;; SHIFTS
;; ----------------------------------------------------------------------
;;
;; We make some attempt to provide real efficient shifting.  One example is
;; doing an 8 bit shift of a 16 bit value by moving a byte reg into the other
;; reg and moving 0 into the former reg.
;;
;; We also try to achieve this in a uniform way.  IE: We don't try to achieve
;; this in both rtl and at insn emit time.  Ideally, we'd use rtl as that would
;; give the optimizer more cracks at the code.  However, we wish to do things
;; like optimizing shifting the sign bit to bit 0 by rotating the other way.
;; There is rtl to handle this (rotate + and), but the H8/300 doesn't handle
;; 16 bit rotates.  Also, if we emit complicated rtl, combine may not be able
;; to detect cases it can optimize.
;;
;; For these and other fuzzy reasons, I've decided to go the less pretty but
;; easier "do it at insn emit time" route.

;; QI BIT SHIFTS

(define_expand "ashlqi3"
  [(set (match_operand:QI 0 "register_operand" "")
	(ashift:QI (match_operand:QI 1 "register_operand" "")
		   (match_operand:QI 2 "nonmemory_operand" "")))]
  ""
  "if (expand_a_shift (QImode, ASHIFT, operands)) DONE; else FAIL;")

(define_expand "ashrqi3"
  [(set (match_operand:QI 0 "register_operand" "")
	(ashiftrt:QI (match_operand:QI 1 "register_operand" "")
		     (match_operand:QI 2 "nonmemory_operand" "")))]
  ""
  "if (expand_a_shift (QImode, ASHIFTRT, operands)) DONE; else FAIL;")

(define_expand "lshrqi3"
  [(set (match_operand:QI 0 "register_operand" "")
	(lshiftrt:QI (match_operand:QI 1 "register_operand" "")
		     (match_operand:QI 2 "nonmemory_operand" "")))]
  ""
  "if (expand_a_shift (QImode, LSHIFTRT, operands)) DONE; else FAIL;")

(define_insn ""
  [(set (match_operand:QI 0 "register_operand" "=r,r")
	(match_operator:QI 3 "nshift_operator"
			[ (match_operand:QI 1 "register_operand" "0,0")
			  (match_operand:QI 2 "nonmemory_operand" "R,rn")]))
   (clobber (match_scratch:QI 4 "=X,&r"))]
  ""
  "* return output_a_shift (operands);"
  [(set (attr "length")
	(symbol_ref "compute_a_shift_length (insn, operands)"))
   (set_attr "cc" "clobber")])

;; HI BIT SHIFTS

(define_expand "ashlhi3"
  [(set (match_operand:HI 0 "register_operand" "")
	(ashift:HI (match_operand:HI 1 "nonmemory_operand" "")
		   (match_operand:QI 2 "nonmemory_operand" "")))]
  ""
  "if (expand_a_shift (HImode, ASHIFT, operands)) DONE; else FAIL;")

(define_expand "lshrhi3"
  [(set (match_operand:HI 0 "register_operand" "")
	(lshiftrt:HI (match_operand:HI 1 "general_operand" "")
		     (match_operand:QI 2 "nonmemory_operand" "")))]
  ""
  "if (expand_a_shift (HImode, LSHIFTRT, operands)) DONE; else FAIL;")

(define_expand "ashrhi3"
  [(set (match_operand:HI 0 "register_operand" "")
	(ashiftrt:HI (match_operand:HI 1 "register_operand" "")
		     (match_operand:QI 2 "nonmemory_operand" "")))]
  ""
  "if (expand_a_shift (HImode, ASHIFTRT, operands)) DONE; else FAIL;")

(define_insn ""
  [(set (match_operand:HI 0 "register_operand" "=r,r")
	(match_operator:HI 3 "nshift_operator"
			[ (match_operand:HI 1 "register_operand" "0,0")
			  (match_operand:QI 2 "nonmemory_operand" "S,rn")]))
   (clobber (match_scratch:QI 4 "=X,&r"))]
  ""
  "* return output_a_shift (operands);"
  [(set (attr "length")
	(symbol_ref "compute_a_shift_length (insn, operands)"))
   (set_attr "cc" "clobber")])

;;  SI BIT SHIFTS

(define_expand "ashlsi3"
  [(set (match_operand:SI 0 "register_operand" "")
	(ashift:SI (match_operand:SI 1 "general_operand" "")
		   (match_operand:QI 2 "nonmemory_operand" "")))]
  ""
  "if (expand_a_shift (SImode, ASHIFT, operands)) DONE; else FAIL;")

(define_expand "lshrsi3"
  [(set (match_operand:SI 0 "register_operand" "")
	(lshiftrt:SI (match_operand:SI 1 "general_operand" "")
		     (match_operand:QI 2 "nonmemory_operand" "")))]
  ""
  "if (expand_a_shift (SImode, LSHIFTRT, operands)) DONE; else FAIL;")

(define_expand "ashrsi3"
  [(set (match_operand:SI 0 "register_operand" "")
	(ashiftrt:SI (match_operand:SI 1 "general_operand" "")
		     (match_operand:QI 2 "nonmemory_operand" "")))]
  ""
  "if (expand_a_shift (SImode, ASHIFTRT, operands)) DONE; else FAIL;")

(define_insn ""
  [(set (match_operand:SI 0 "register_operand" "=r,r")
	(match_operator:SI 3 "nshift_operator"
			[ (match_operand:SI 1 "register_operand" "0,0")
			  (match_operand:QI 2 "nonmemory_operand" "T,rn")]))
   (clobber (match_scratch:QI 4 "=X,&r"))]
  ""
  "* return output_a_shift (operands);"
  [(set (attr "length")
	(symbol_ref "compute_a_shift_length (insn, operands)"))
   (set_attr "cc" "clobber")])

;; ----------------------------------------------------------------------
;; ROTATIONS
;; ----------------------------------------------------------------------

(define_expand "rotlqi3"
  [(set (match_operand:QI 0 "register_operand" "")
	(rotate:QI (match_operand:QI 1 "register_operand" "")
		   (match_operand:QI 2 "nonmemory_operand" "")))]
  ""
  "if (expand_a_rotate (ROTATE, operands)) DONE; else FAIL;")

(define_insn "*rotlqi3_1"
  [(set (match_operand:QI 0 "register_operand" "=r")
	(rotate:QI (match_operand:QI 1 "register_operand" "0")
		   (match_operand:QI 2 "immediate_operand" "")))]
  ""
  "* return emit_a_rotate (ROTATE, operands);"
  [(set_attr "length" "20")
   (set_attr "cc" "clobber")])

(define_expand "rotlhi3"
  [(set (match_operand:HI 0 "register_operand" "")
	(rotate:HI (match_operand:HI 1 "register_operand" "")
		   (match_operand:QI 2 "nonmemory_operand" "")))]
  ""
  "if (expand_a_rotate (ROTATE, operands)) DONE; else FAIL;")

(define_insn "*rotlhi3_1"
  [(set (match_operand:HI 0 "register_operand" "=r")
	(rotate:HI (match_operand:HI 1 "register_operand" "0")
		   (match_operand:QI 2 "immediate_operand" "")))]
  ""
  "* return emit_a_rotate (ROTATE, operands);"
  [(set_attr "length" "20")
   (set_attr "cc" "clobber")])

(define_expand "rotlsi3"
  [(set (match_operand:SI 0 "register_operand" "")
	(rotate:SI (match_operand:SI 1 "register_operand" "")
		   (match_operand:QI 2 "nonmemory_operand" "")))]
  "TARGET_H8300H || TARGET_H8300S"
  "if (expand_a_rotate (ROTATE, operands)) DONE; else FAIL;")

(define_insn "*rotlsi3_1"
  [(set (match_operand:SI 0 "register_operand" "=r")
	(rotate:SI (match_operand:SI 1 "register_operand" "0")
		   (match_operand:QI 2 "immediate_operand" "")))]
  "TARGET_H8300H || TARGET_H8300S"
  "* return emit_a_rotate (ROTATE, operands);"
  [(set_attr "length" "20")
   (set_attr "cc" "clobber")])

;; -----------------------------------------------------------------
;; BIT FIELDS
;; -----------------------------------------------------------------
;; The H8/300 has given 1/8th of its opcode space to bitfield
;; instructions so let's use them as well as we can.

;; You'll never believe all these patterns perform one basic action --
;; load a bit from the source, optionally invert the bit, then store it
;; in the destination (which is known to be zero).
;;
;; Combine obviously need some work to better identify this situation and
;; canonicalize the form better.

;;
;; Normal loads with a 16bit destination.
;;

(define_insn ""
  [(set (match_operand:HI 0 "register_operand" "=&r")
	(zero_extract:HI (match_operand:HI 1 "register_operand" "r")
			 (const_int 1)
			 (match_operand:HI 2 "immediate_operand" "n")))]
  "TARGET_H8300"
  "sub.w	%0,%0\;bld	%Z2,%Y1\;bst	#0,%X0"
  [(set_attr "cc" "clobber")
   (set_attr "length" "6")])

;;
;; Inverted loads with a 16bit destination.
;;

(define_insn ""
  [(set (match_operand:HI 0 "register_operand" "=&r")
	(zero_extract:HI (xor:HI (match_operand:HI 1 "register_operand" "r")
				 (match_operand:HI 3 "const_int_operand" "n"))
			 (const_int 1)
			 (match_operand:HI 2 "const_int_operand" "n")))]
  "TARGET_H8300
   && (1 << INTVAL (operands[2])) == INTVAL (operands[3])"
  "sub.w	%0,%0\;bild	%Z2,%Y1\;bst	#0,%X0"
  [(set_attr "cc" "clobber")
   (set_attr "length" "8")])

;;
;; Normal loads with a 32bit destination.
;;

(define_insn "*extzv_1_r_h8300"
  [(set (match_operand:SI 0 "register_operand" "=&r")
	(zero_extract:SI (match_operand:HI 1 "register_operand" "r")
			 (const_int 1)
			 (match_operand 2 "const_int_operand" "n")))]
  "TARGET_H8300
   && INTVAL (operands[2]) < 16"
  "* return output_simode_bld (0, operands);"
  [(set_attr "cc" "clobber")
   (set_attr "length" "8")])

(define_insn "*extzv_1_r_h8300hs"
  [(set (match_operand:SI 0 "register_operand" "=r")
	(zero_extract:SI (match_operand:SI 1 "register_operand" "r")
			 (const_int 1)
			 (match_operand 2 "const_int_operand" "n")))]
  "(TARGET_H8300H || TARGET_H8300S)
   && INTVAL (operands[2]) < 16"
  "* return output_simode_bld (0, operands);"
  [(set_attr "cc" "clobber")
   (set_attr "length" "8")])

;;
;; Inverted loads with a 32bit destination.
;;

(define_insn "*extzv_1_r_inv_h8300"
  [(set (match_operand:SI 0 "register_operand" "=&r")
	(zero_extract:SI (xor:HI (match_operand:HI 1 "register_operand" "r")
				 (match_operand:HI 3 "const_int_operand" "n"))
			 (const_int 1)
			 (match_operand 2 "const_int_operand" "n")))]
  "TARGET_H8300
   && INTVAL (operands[2]) < 16
   && (1 << INTVAL (operands[2])) == INTVAL (operands[3])"
  "* return output_simode_bld (1, operands);"
  [(set_attr "cc" "clobber")
   (set_attr "length" "8")])

(define_insn "*extzv_1_r_inv_h8300hs"
  [(set (match_operand:SI 0 "register_operand" "=r")
	(zero_extract:SI (xor:SI (match_operand:SI 1 "register_operand" "r")
				 (match_operand 3 "const_int_operand" "n"))
			 (const_int 1)
			 (match_operand 2 "const_int_operand" "n")))]
  "(TARGET_H8300H || TARGET_H8300S)
   && INTVAL (operands[2]) < 16
   && (1 << INTVAL (operands[2])) == INTVAL (operands[3])"
  "* return output_simode_bld (1, operands);"
  [(set_attr "cc" "clobber")
   (set_attr "length" "8")])

(define_expand "insv"
  [(set (zero_extract:HI (match_operand:HI 0 "general_operand" "")
			 (match_operand:HI 1 "general_operand" "")
			 (match_operand:HI 2 "general_operand" ""))
	(match_operand:HI 3 "general_operand" ""))]
  "TARGET_H8300"
  "
{
  /* We only have single bit bit-field instructions.  */
  if (INTVAL (operands[1]) != 1)
    FAIL;

  /* For now, we don't allow memory operands.  */
  if (GET_CODE (operands[0]) == MEM
      || GET_CODE (operands[3]) == MEM)
    FAIL;
}")

(define_insn ""
  [(set (zero_extract:HI (match_operand:HI 0 "register_operand" "+r")
			 (const_int 1)
			 (match_operand:HI 1 "immediate_operand" "n"))
	(match_operand:HI 2 "register_operand" "r"))]
  ""
  "bld	#0,%R2\;bst	%Z1,%Y0 ; i1"
  [(set_attr "cc" "clobber")
   (set_attr "length" "4")])

(define_expand "extzv"
  [(set (match_operand:HI 0 "register_operand" "")
	(zero_extract:HI (match_operand:HI 1 "bit_operand" "")
			 (match_operand:HI 2 "general_operand" "")
			 (match_operand:HI 3 "general_operand" "")))]
  "TARGET_H8300"
  "
{
  /* We only have single bit bit-field instructions.  */
  if (INTVAL (operands[2]) != 1)
    FAIL;

  /* For now, we don't allow memory operands.  */
  if (GET_CODE (operands[1]) == MEM)
    FAIL;
}")

;; BAND, BOR, and BXOR patterns

(define_insn ""
  [(set (match_operand:HI 0 "bit_operand" "=Ur")
	(match_operator:HI 4 "bit_operator"
	   [(zero_extract:HI (match_operand:HI 1 "register_operand" "r")
			     (const_int 1)
			     (match_operand:HI 2 "immediate_operand" "n"))
	    (match_operand:HI 3 "bit_operand" "0")]))]
  ""
  "bld	%Z2,%Y1\;%b4	#0,%R0\;bst	#0,%R0; bl1"
  [(set_attr "cc" "clobber")
   (set_attr "length" "6")
   (set_attr "adjust_length" "no")])

(define_insn ""
  [(set (match_operand:HI 0 "bit_operand" "=Ur")
	(match_operator:HI 5 "bit_operator"
	   [(zero_extract:HI (match_operand:HI 1 "register_operand" "r")
			     (const_int 1)
			     (match_operand:HI 2 "immediate_operand" "n"))
	    (zero_extract:HI (match_operand:HI 3 "register_operand" "r")
			     (const_int 1)
			     (match_operand:HI 4 "immediate_operand" "n"))]))]
  ""
  "bld	%Z2,%Y1\;%b5	%Z4,%Y3\;bst	#0,%R0; bl3"
  [(set_attr "cc" "clobber")
   (set_attr "length" "6")
   (set_attr "adjust_length" "no")])

;; -----------------------------------------------------------------
;; COMBINE PATTERNS
;; -----------------------------------------------------------------

(define_insn "*extzv_8_8"
  [(set (match_operand:SI 0 "register_operand" "=r")
	(zero_extract:SI (match_operand:SI 1 "register_operand" "r")
			 (const_int 8)
			 (const_int 8)))]
  "TARGET_H8300H || TARGET_H8300S"
  "mov.b\\t%x1,%w0\;extu.w\\t%f0\;extu.l\\t%S0"
  [(set_attr "cc" "set_znv")
   (set_attr "length" "6")])

(define_insn "*extzv_8_16"
  [(set (match_operand:SI 0 "register_operand" "=r")
	(zero_extract:SI (match_operand:SI 1 "register_operand" "r")
			 (const_int 8)
			 (const_int 16)))]
  "TARGET_H8300H || TARGET_H8300S"
  "mov.w\\t%e1,%f0\;extu.w\\t%f0\;extu.l\\t%S0"
  [(set_attr "cc" "set_znv")
   (set_attr "length" "6")])

(define_insn ""
  [(set (match_operand:HI 0 "register_operand" "=r")
	(ior:HI (zero_extend:HI (match_operand:QI 1 "register_operand" "r"))
		(match_operand:HI 2 "register_operand" "0")))]
  "REG_P (operands[0])
   && REG_P (operands[1])
   && REGNO (operands[0]) != REGNO (operands[1])"
  "or\\t%X1,%s0"
  [(set_attr "cc" "clobber")
   (set_attr "length" "2")])

(define_insn ""
  [(set (match_operand:SI 0 "register_operand" "=r")
	(ior:SI (zero_extend:SI (match_operand:HI 1 "register_operand" "r"))
		(match_operand:SI 2 "register_operand" "0")))]
  "(TARGET_H8300H || TARGET_H8300S)
   && REG_P (operands[0])
   && REG_P (operands[1])
   && (REGNO (operands[0]) != REGNO (operands[1]))"
  "or.w\\t%T1,%f0"
  [(set_attr "cc" "clobber")
   (set_attr "length" "2")])

(define_insn ""
  [(set (match_operand:SI 0 "register_operand" "=r")
	(ior:SI (zero_extend:SI (match_operand:QI 1 "register_operand" "r"))
		(match_operand:SI 2 "register_operand" "0")))]
  ""
  "or\\t%X1,%w0"
  [(set_attr "cc" "clobber")
   (set_attr "length" "2")])

(define_insn ""
  [(set (match_operand:HI 0 "register_operand" "=r")
	(xor:HI (zero_extend:HI (match_operand:QI 1 "register_operand" "r"))
		(match_operand:HI 2 "register_operand" "0")))]
  "REG_P (operands[0])
   && REG_P (operands[1])
   && REGNO (operands[0]) != REGNO (operands[1])"
  "xor\\t%X1,%s0"
  [(set_attr "cc" "clobber")
   (set_attr "length" "2")])

(define_insn ""
  [(set (match_operand:SI 0 "register_operand" "=r")
	(xor:SI (zero_extend:SI (match_operand:HI 1 "register_operand" "r"))
		(match_operand:SI 2 "register_operand" "0")))]
  "(TARGET_H8300H || TARGET_H8300S)
   && REG_P (operands[0])
   && REG_P (operands[1])
   && (REGNO (operands[0]) != REGNO (operands[1]))"
  "xor.w\\t%T1,%f0"
  [(set_attr "cc" "clobber")
   (set_attr "length" "2")])

(define_insn ""
  [(set (match_operand:SI 0 "register_operand" "=r")
	(xor:SI (zero_extend:SI (match_operand:QI 1 "register_operand" "r"))
		(match_operand:SI 2 "register_operand" "0")))]
  "REG_P (operands[0])
   && REG_P (operands[1])
   && REGNO (operands[0]) != REGNO (operands[1])"
  "xor\\t%X1,%w0"
  [(set_attr "cc" "clobber")
   (set_attr "length" "2")])

(define_insn ""
  [(set (match_operand:HI 0 "register_operand" "=r")
	(ior:HI (zero_extend:HI (match_operand:QI 1 "register_operand" "0"))
		(ashift:HI (match_operand:HI 2 "register_operand" "r")
			   (const_int 8))))]
  "REG_P (operands[0])
   && REG_P (operands[2])
   && REGNO (operands[0]) != REGNO (operands[2])"
  "mov.b\\t%s2,%t0"
  [(set_attr "cc" "clobber")
   (set_attr "length" "2")])

(define_insn "*iorhi_shift_8"
  [(set (match_operand:HI 0 "register_operand" "=r")
	(ior:HI (ashift:HI (match_operand:HI 1 "register_operand" "r")
			   (const_int 8))
		(match_operand:HI 2 "register_operand" "0")))]
  ""
  "or.b\\t%s1,%t0"
  [(set_attr "cc" "clobber")
   (set_attr "length" "2")])

(define_insn ""
  [(set (match_operand:SI 0 "register_operand" "=r")
	(ior:SI (zero_extend:SI (match_operand:HI 1 "register_operand" "0"))
		(ashift:SI (match_operand:SI 2 "register_operand" "r")
			   (const_int 16))))]
  "TARGET_H8300H || TARGET_H8300S"
  "mov.w\\t%f2,%e0"
  [(set_attr "cc" "clobber")
   (set_attr "length" "2")])

(define_insn ""
  [(set (match_operand:SI 0 "register_operand" "=r")
	(ior:SI (ashift:SI (match_operand:SI 1 "register_operand" "r")
			   (const_int 16))
		(match_operand:SI 2 "register_operand" "0")))]
  "TARGET_H8300H || TARGET_H8300S"
  "or.w\\t%f1,%e0"
  [(set_attr "cc" "clobber")
   (set_attr "length" "2")])

;; Storing a part of HImode to QImode.

(define_insn ""
  [(set (match_operand:QI 0 "general_operand_dst" "=rm<")
	(subreg:QI (lshiftrt:HI (match_operand:HI 1 "register_operand" "r")
				(const_int 8)) 1))]
  ""
  "mov.b\\t%t1,%R0"
  [(set_attr "cc" "set_znv")
   (set_attr "length" "8")])

;; Storing a part of SImode to QImode.

(define_insn ""
  [(set (match_operand:QI 0 "general_operand_dst" "=rm<")
	(subreg:QI (lshiftrt:SI (match_operand:SI 1 "register_operand" "r")
				(const_int 8)) 3))]
  ""
  "mov.b\\t%x1,%R0"
  [(set_attr "cc" "set_znv")
   (set_attr "length" "8")])

(define_insn ""
  [(set (match_operand:QI 0 "general_operand_dst" "=rm<")
	(subreg:QI (lshiftrt:SI (match_operand:SI 1 "register_operand" "r")
				(const_int 16)) 3))
   (clobber (match_scratch:SI 2 "=&r"))]
  "TARGET_H8300H || TARGET_H8300S"
  "mov.w\\t%e1,%f2\;mov.b\\t%w2,%R0"
  [(set_attr "cc" "set_znv")
   (set_attr "length" "10")])

(define_insn ""
  [(set (match_operand:QI 0 "general_operand_dst" "=rm<")
	(subreg:QI (lshiftrt:SI (match_operand:SI 1 "register_operand" "r")
				(const_int 24)) 3))
   (clobber (match_scratch:SI 2 "=&r"))]
  "TARGET_H8300H || TARGET_H8300S"
  "mov.w\\t%e1,%f2\;mov.b\\t%x2,%R0"
  [(set_attr "cc" "set_znv")
   (set_attr "length" "10")])

(define_insn_and_split ""
  [(set (pc)
	(if_then_else (eq (zero_extract:SI (subreg:SI (match_operand:QI 0 "register_operand" "") 0)
					   (const_int 1)
					   (const_int 7))
			  (const_int 0))
		      (label_ref (match_operand 1 "" ""))
		      (pc)))]
  ""
  "#"
  ""
  [(set (cc0)
	(match_dup 0))
   (set (pc)
	(if_then_else (ge (cc0)
			  (const_int 0))
		      (label_ref (match_dup 1))
		      (pc)))]
  "")

(define_insn_and_split ""
  [(set (pc)
	(if_then_else (ne (zero_extract:SI (subreg:SI (match_operand:QI 0 "register_operand" "") 0)
					   (const_int 1)
					   (const_int 7))
			  (const_int 0))
		      (label_ref (match_operand 1 "" ""))
		      (pc)))]
  ""
  "#"
  ""
  [(set (cc0)
	(match_dup 0))
   (set (pc)
	(if_then_else (lt (cc0)
			  (const_int 0))
		      (label_ref (match_dup 1))
		      (pc)))]
  "")

;; -----------------------------------------------------------------
;; PEEPHOLE PATTERNS
;; -----------------------------------------------------------------

;; Convert (A >> B) & C to (A & 255) >> B if C == 255 >> B.

(define_peephole2
  [(parallel
     [(set (match_operand:HI 0 "register_operand" "")
	   (lshiftrt:HI (match_dup 0)
			(match_operand:HI 1 "const_int_operand" "")))
      (clobber (match_operand:HI 2 "" ""))])
   (set (match_dup 0)
	(and:HI (match_dup 0)
		(match_operand:HI 3 "const_int_operand" "")))]
  "INTVAL (operands[3]) == (255 >> INTVAL (operands[1]))"
  [(set (match_dup 0)
	(and:HI (match_dup 0)
		(const_int 255)))
   (parallel
     [(set (match_dup 0)
	   (lshiftrt:HI (match_dup 0)
			(match_dup 1)))
      (clobber (match_dup 2))])]
  "")

;; Convert (A << B) & C to (A & 255) << B if C == 255 << B.

(define_peephole2
  [(parallel
     [(set (match_operand:HI 0 "register_operand" "")
	   (ashift:HI (match_dup 0)
		      (match_operand:HI 1 "const_int_operand" "")))
      (clobber (match_operand:HI 2 "" ""))])
   (set (match_dup 0)
	(and:HI (match_dup 0)
		(match_operand:HI 3 "const_int_operand" "")))]
  "INTVAL (operands[3]) == (255 << INTVAL (operands[1]))"
  [(set (match_dup 0)
	(and:HI (match_dup 0)
		(const_int 255)))
   (parallel
     [(set (match_dup 0)
	   (ashift:HI (match_dup 0)
		      (match_dup 1)))
      (clobber (match_dup 2))])]
  "")

;; Convert (A >> B) & C to (A & 255) >> B if C == 255 >> B.

(define_peephole2
  [(parallel
     [(set (match_operand:SI 0 "register_operand" "")
	   (lshiftrt:SI (match_dup 0)
			(match_operand:SI 1 "const_int_operand" "")))
      (clobber (match_operand:SI 2 "" ""))])
   (set (match_dup 0)
	(and:SI (match_dup 0)
		(match_operand:SI 3 "const_int_operand" "")))]
  "INTVAL (operands[3]) == (255 >> INTVAL (operands[1]))"
  [(set (match_dup 0)
	(and:SI (match_dup 0)
		(const_int 255)))
   (parallel
     [(set (match_dup 0)
	   (lshiftrt:SI (match_dup 0)
			(match_dup 1)))
      (clobber (match_dup 2))])]
  "")

;; Convert (A << B) & C to (A & 255) << B if C == 255 << B.

(define_peephole2
  [(parallel
     [(set (match_operand:SI 0 "register_operand" "")
	   (ashift:SI (match_dup 0)
		      (match_operand:SI 1 "const_int_operand" "")))
      (clobber (match_operand:SI 2 "" ""))])
   (set (match_dup 0)
	(and:SI (match_dup 0)
		(match_operand:SI 3 "const_int_operand" "")))]
  "INTVAL (operands[3]) == (255 << INTVAL (operands[1]))"
  [(set (match_dup 0)
	(and:SI (match_dup 0)
		(const_int 255)))
   (parallel
     [(set (match_dup 0)
	   (ashift:SI (match_dup 0)
		      (match_dup 1)))
      (clobber (match_dup 2))])]
  "")

;; Convert (A >> B) & C to (A & 65535) >> B if C == 65535 >> B.

(define_peephole2
  [(parallel
     [(set (match_operand:SI 0 "register_operand" "")
	   (lshiftrt:SI (match_dup 0)
			(match_operand:SI 1 "const_int_operand" "")))
      (clobber (match_operand:SI 2 "" ""))])
   (set (match_dup 0)
	(and:SI (match_dup 0)
		(match_operand:SI 3 "const_int_operand" "")))]
  "INTVAL (operands[3]) == (65535 >> INTVAL (operands[1]))"
  [(set (match_dup 0)
	(and:SI (match_dup 0)
		(const_int 65535)))
   (parallel
     [(set (match_dup 0)
	   (lshiftrt:SI (match_dup 0)
			(match_dup 1)))
      (clobber (match_dup 2))])]
  "")

;; Convert (A << B) & C to (A & 65535) << B if C == 65535 << B.

(define_peephole2
  [(parallel
     [(set (match_operand:SI 0 "register_operand" "")
	   (ashift:SI (match_dup 0)
		      (match_operand:SI 1 "const_int_operand" "")))
      (clobber (match_operand:SI 2 "" ""))])
   (set (match_dup 0)
	(and:SI (match_dup 0)
		(match_operand:SI 3 "const_int_operand" "")))]
  "INTVAL (operands[3]) == (65535 << INTVAL (operands[1]))"
  [(set (match_dup 0)
	(and:SI (match_dup 0)
		(const_int 65535)))
   (parallel
     [(set (match_dup 0)
	   (ashift:SI (match_dup 0)
		      (match_dup 1)))
      (clobber (match_dup 2))])]
  "")

;; Convert a QImode push into an SImode push so that the
;; define_peephole2 below can cram multiple pushes into one stm.l.

(define_peephole2
  [(parallel [(set (reg:SI SP_REG)
                   (plus:SI (reg:SI SP_REG) (const_int -4)))
              (set (mem:QI (plus:SI (reg:SI SP_REG) (const_int -3)))
                   (match_operand:QI 0 "register_operand" ""))])]
  "TARGET_H8300S"
  [(set (mem:SI (pre_dec:SI (reg:SI SP_REG)))
	(match_dup 0))]
  "operands[0] = gen_rtx_REG (SImode, REGNO (operands[0]));")

;; Convert a HImode push into an SImode push so that the
;; define_peephole2 below can cram multiple pushes into one stm.l.

(define_peephole2
  [(parallel [(set (reg:SI SP_REG)
                   (plus:SI (reg:SI SP_REG) (const_int -4)))
              (set (mem:HI (plus:SI (reg:SI SP_REG) (const_int -2)))
                   (match_operand:HI 0 "register_operand" ""))])]
  "TARGET_H8300S"
  [(set (mem:SI (pre_dec:SI (reg:SI SP_REG)))
	(match_dup 0))]
  "operands[0] = gen_rtx_REG (SImode, REGNO (operands[0]));")

;; Cram four pushes into stm.l.

(define_peephole2
  [(set (mem:SI (pre_dec:SI (reg:SI SP_REG)))
	(match_operand:SI 0 "register_operand" ""))
   (set (mem:SI (pre_dec:SI (reg:SI SP_REG)))
	(match_operand:SI 1 "register_operand" ""))
   (set (mem:SI (pre_dec:SI (reg:SI SP_REG)))
	(match_operand:SI 2 "register_operand" ""))
   (set (mem:SI (pre_dec:SI (reg:SI SP_REG)))
	(match_operand:SI 3 "register_operand" ""))]
  "TARGET_H8300S
   && REGNO (operands[0]) == 0
   && REGNO (operands[1]) == 1
   && REGNO (operands[2]) == 2
   && REGNO (operands[3]) == 3"
  [(parallel [(set (reg:SI SP_REG)
		   (plus:SI (reg:SI SP_REG)
			    (const_int -16)))
	      (set (mem:SI (plus:SI (reg:SI SP_REG) (const_int -4)))
		   (match_dup 0))
	      (set (mem:SI (plus:SI (reg:SI SP_REG) (const_int -8)))
		   (match_dup 1))
	      (set (mem:SI (plus:SI (reg:SI SP_REG) (const_int -12)))
		   (match_dup 2))
	      (set (mem:SI (plus:SI (reg:SI SP_REG) (const_int -16)))
		   (match_dup 3))])]
  "")

;; Cram three pushes into stm.l.

(define_peephole2
  [(set (mem:SI (pre_dec:SI (reg:SI SP_REG)))
	(match_operand:SI 0 "register_operand" ""))
   (set (mem:SI (pre_dec:SI (reg:SI SP_REG)))
	(match_operand:SI 1 "register_operand" ""))
   (set (mem:SI (pre_dec:SI (reg:SI SP_REG)))
	(match_operand:SI 2 "register_operand" ""))]
  "TARGET_H8300S
   && ((REGNO (operands[0]) == 0
	&& REGNO (operands[1]) == 1
	&& REGNO (operands[2]) == 2)
       || (REGNO (operands[0]) == 4
	   && REGNO (operands[1]) == 5
	   && REGNO (operands[2]) == 6))"
  [(parallel [(set (reg:SI SP_REG)
		   (plus:SI (reg:SI SP_REG)
			    (const_int -12)))
	      (set (mem:SI (plus:SI (reg:SI SP_REG) (const_int -4)))
		   (match_dup 0))
	      (set (mem:SI (plus:SI (reg:SI SP_REG) (const_int -8)))
		   (match_dup 1))
	      (set (mem:SI (plus:SI (reg:SI SP_REG) (const_int -12)))
		   (match_dup 2))])]
  "")

;; Cram two pushes into stm.l.

(define_peephole2
  [(set (mem:SI (pre_dec:SI (reg:SI SP_REG)))
	(match_operand:SI 0 "register_operand" ""))
   (set (mem:SI (pre_dec:SI (reg:SI SP_REG)))
	(match_operand:SI 1 "register_operand" ""))]
  "TARGET_H8300S
   && ((REGNO (operands[0]) == 0 && REGNO (operands[1]) == 1)
       || (REGNO (operands[0]) == 2 && REGNO (operands[1]) == 3)
       || (REGNO (operands[0]) == 4 && REGNO (operands[1]) == 5))"
  [(parallel [(set (reg:SI SP_REG)
		   (plus:SI (reg:SI SP_REG)
			    (const_int -8)))
	      (set (mem:SI (plus:SI (reg:SI SP_REG) (const_int -4)))
		   (match_dup 0))
	      (set (mem:SI (plus:SI (reg:SI SP_REG) (const_int -8)))
		   (match_dup 1))])]
  "")

;; Turn
;;
;;   mov.w #2,r0
;;   add.w r7,r0  (6 bytes)
;;
;; into
;;
;;   mov.w r7,r0
;;   adds  #2,r0  (4 bytes)

(define_peephole2
  [(set (match_operand:HI 0 "register_operand" "")
	(match_operand:HI 1 "const_int_operand" ""))
   (set (match_dup 0)
	(plus:HI (match_dup 0)
		 (match_operand:HI 2 "register_operand" "")))]
  "REG_P (operands[0]) && REG_P (operands[2])
   && REGNO (operands[0]) != REGNO (operands[2])
   && (CONST_OK_FOR_J (INTVAL (operands[1]))
       || CONST_OK_FOR_L (INTVAL (operands[1]))
       || CONST_OK_FOR_N (INTVAL (operands[1])))"
  [(set (match_dup 0)
	(match_dup 2))
   (set (match_dup 0)
	(plus:HI (match_dup 0)
		 (match_dup 1)))]
  "")

;; Turn
;;
;;   sub.l  er0,er0
;;   add.b  #4,r0l
;;   add.l  er7,er0  (6 bytes)
;;
;; into
;;
;;   mov.l  er7,er0
;;   adds   #4,er0   (4 bytes)

(define_peephole2
  [(set (match_operand:SI 0 "register_operand" "")
	(match_operand:SI 1 "const_int_operand" ""))
   (set (match_dup 0)
	(plus:SI (match_dup 0)
		 (match_operand:SI 2 "register_operand" "")))]
  "(TARGET_H8300H || TARGET_H8300S)
   && REG_P (operands[0]) && REG_P (operands[2])
   && REGNO (operands[0]) != REGNO (operands[2])
   && (CONST_OK_FOR_L (INTVAL (operands[1]))
       || CONST_OK_FOR_N (INTVAL (operands[1])))"
  [(set (match_dup 0)
	(match_dup 2))
   (set (match_dup 0)
	(plus:SI (match_dup 0)
		 (match_dup 1)))]
  "")

;; Turn
;;
;;   mov.l er7,er0
;;   add.l #10,er0  (takes 8 bytes)
;;
;; into
;;
;;   sub.l er0,er0
;;   add.b #10,r0l
;;   add.l er7,er0  (takes 6 bytes)

(define_peephole2
  [(set (match_operand:SI 0 "register_operand" "")
	(match_operand:SI 1 "register_operand" ""))
   (set (match_dup 0)
	(plus:SI (match_dup 0)
		 (match_operand:SI 2 "const_int_operand" "")))]
  "(TARGET_H8300H || TARGET_H8300S)
   && REG_P (operands[0]) && REG_P (operands[1])
   && REGNO (operands[0]) != REGNO (operands[1])
   && !CONST_OK_FOR_L (INTVAL (operands[2]))
   && !CONST_OK_FOR_N (INTVAL (operands[2]))
   && ((INTVAL (operands[2]) & 0xff) == INTVAL (operands[2])
       || (INTVAL (operands[2]) & 0xff00) == INTVAL (operands[2])
       || INTVAL (operands[2]) == 0xffff
       || INTVAL (operands[2]) == 0xfffe)"
  [(set (match_dup 0)
	(match_dup 2))
   (set (match_dup 0)
	(plus:SI (match_dup 0)
		 (match_dup 1)))]
  "")
